Hot Swap and Power Monitor Evaluation Software
This software can be used to communicate with the ADM1275, ADM1276 and ADM1075 Hot Swap and Power Monitor devices using an I2C interface. A supported hardware interface must be used to provide an I2C interface to the part, such as the ADI USB to I2C cable (USB-SMBUS-CABLEZ).

Important Notice: I2C Interface Cables Device Drivers Requirements
The evaluation software supports the following USB to I2C interface cables:
•	USB-SMBUS-CABLEZ
•	USB-SDP-CABLEZ

The ADMxxxx Run-Time installs the necessary devices drivers to support these interfaces on the PC for use with the ADI evaluation tools.  These devices drivers support the Microsoft Windows XP, Vista, and 7 versions of the operating system.

If you have previously used the USB-SMBUS-CABLEZ or USB-5PSMBUS-CABLEZ with one of the following versions, or previous versions of the evaluation software, then you must also remove an older version of the device driver for these interface cables.
•	ADM106x Configuration Tool v4.0.6
•	ADM106x prog106x command line Tool v.1.0.2
•	ADM1175-8/91-92 Configuration Tool v 3.0.1

Refer to the document 'Updating USB-IIC Dongle Driver' in the Common folder of the Analog Devices entry in the Start menu for more details.

The CABLE-SMBUS-3PINZ and CABLE-SMBUS-5PINZ are Parallel port to IIC converter cables.  These are not supported by this software.

Minimum system requirements
Windows XP SP2
1 GHz Processor
200 Meg free disc space
512Mb RAM

Minimum viewing resolution
1024 x 768 High color (16 bit)

Version History
1.3.2	Fixed a problem with the software searching for a missing DLL file at the startup. 

1.3.1	Fixed a problem with detecting I2C interfaces, where if the USB-SDP-CABLEZ interface had never been connected to a PC, it could prevent other I2C interfaces from being detected.

1.3.0	Added support for the USB-SDP-CABLEZ Interface cable

1.2.0	Support added for the ADM1075 family of parts.

Known Issues:
•	Holding down the Energy Metering display mode select pop-up menu for longer than a few seconds may delay updates from the device being read, and result in incorrect energy usage being reported.

1.1.0	Renamed the tool to Hot Swap & Power Monitor Evaluation software as it now supports the ADM1275 and ADM1276

1.0.1	Changed Number Conversion tab to include only valid options.

1.0.0	Initial Release