Contact Information:

Eric Trelewicz
Linear Technology
408-432-1900 x3006
Email etrelewicz@linear.com

Instructions:

Please provide quotes for the following  quantity:
At least 10 board rounded to the nearest panel
5 and 10 day delivery


Fabricate per notes on the DC997B2.fab drawing.

PAY SPECIAL ATTENTION TO CENTERING EDGE CONNECTOR PATTERN ON ALIGNMENT NOTCH! 
THIS EDGE CONNECTOR HAS A FINE PITCH IT IS IMPORTANT FOR THE COPPER PATTERN 
ON TOP AND BOTTOM TO BE CLOSELY ALLIGNED AND CENTERED AROUND THE NOTCH.


All photo data is provided in geber 274X format.
Drill information is provided in echellon format.
Summary files are in ASCII text format.

PDF versions of the artwork (1:1 and 2:1) and the fabrication drawing 
are provided for convenience. 

All layers viewed from top unless noted below!

File Extensions:

	.spt	solder paste top
	.spb	solder paste bottom
	.sst	silkscreen top
	.ssb	sildscreen bottom
	.smt	solder mask top
	.smb	solder mask bottom
	.l1	layer 1 (Top)	positive
	.l2	layer 2		positive
	.l3	layer 3		positive
	.l4	layer 4         positive
        .l5     layer 5         positive
        .l6     layer 6 (Bottom)positive
	.gpi	Gerber photo ploter information
	.tap	Echellon drill file
	.dri	Drill station information
	.drl	Drill Rack (data in inches)
	.FAB	fabrication drawing
	.ast	assembly top
	.asb	assembly bottom (MIRRORED) 