************************************************************************************

This ZIP File is associated with Rev 1 of the Application Note

	Host DMA PORT on ADSP-BF52x and ADSP-BF54x Blackfin® Processors (EE-337)

that can be found at http://www.analog.com/ee-notes

Date Created:   May 6, 2008


************************************************************************************


This folder contains the sample codes for both Acknowledge Mode and Interrupt Mode
in C and Assembly. Refer to the readme.txt in respective folders for more details.


************************************************************************************


All the code examples have been written and tested with

	VisualDSP++ 5.0 (Feb 2008 update)

	ADSP-BF537 rev 0.3, 
	ADSP-BF537 EZ-Kit Lite Rev 1.3
	
	ADSP-BF527 rev 0.0, 
	ADSP-BF527 EZ-Kit Lite Rev 1.4

	ADSP-BF548 rev 0.0, 
	ADSP-BF548 EZ-Kit Lite Rev 1.3


