The ADA4961 eval board requires the Analog Devices SDP-S USB interface board, available from the ADI website at www.analog.com/sdp.

Connect the SDP-S USB interface board to the ADA4961 eval board. Connect the USBcable from the PC to the SDP-S adapter board. Apply 5V and input and output cables to the ADA4961. These steps do not have to be done in any specific order.

Installation instructions for ADA4961, rev 0p0p0 software;
1. Extract .zip file
2. Run SDP driver installer, SDPDrivers.exe
3. Run ADA4961 customer software installer, ADA4961_0p0p0_installer.exe

An Analog Devices icon should appear on the user desktop, with the title ADA4961. Click on this icon to run the ADA4961 customer software GUI. 