| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - g -

- g16 : DC1410AB.ino , DC1410AA.ino
- g32 : DC1410AA.ino , DC1410AB.ino
- g8 : DC1410AB.ino , DC1410AA.ino
- GENERIC_GPIO : platform_drivers.h
- GENERIC_I2C : platform_drivers.h
- GENERIC_SPI : platform_drivers.h
- get_char() : DC590B.ino , DC590B_enhanced.ino , DC590_subset.ino , DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino , DC2430A.ino
- get_code() : DC2376A.ino , DC2196A.ino , DC2025A.ino , DC579A.ino , DC809A.ino , DC935A.ino , DC934A.ino , DC1466.ino , DC1534A.ino , DC1333A.ino , DC1096B.ino , DC2197.ino , DC1678A.ino , DC1703A.ino , DC1397A.ino , DC1529A.ino , DC2692A.ino
- get_current() : DC2692A.ino
- get_filtered_hex_data() : nvm.cpp
- get_hex_data() : nvm.cpp
- get_LTC6945_global_fref_Hz() : LTC6945.cpp , LTC6945.h
- get_LTC6945_global_fref_MHz() : LTC6945.cpp , LTC6945.h
- get_LTC6945_global_frf_Hz() : LTC6945.cpp , LTC6945.h
- get_LTC6945_global_frf_MHz() : LTC6945.cpp , LTC6945.h
- get_LTC6945_global_VCO_MAX_Hz() : LTC6945.cpp , LTC6945.h
- get_LTC6945_global_VCO_MAX_MHz() : LTC6945.cpp , LTC6945.h
- get_LTC6945_global_VCO_MIN_Hz() : LTC6945.cpp , LTC6945.h
- get_LTC6945_global_VCO_MIN_MHz() : LTC6945.cpp , LTC6945.h
- get_LTC6945_REGSIZE() : LTC6945.cpp , LTC6945.h
- get_LTC6945_SPI_FIELD() : LTC6945.cpp , LTC6945.h
- get_LTC6945_SPI_FIELD_NUMBITS() : LTC6945.cpp , LTC6945.h
- get_LTC6945_SPI_FIELD_RW() : LTC6945.cpp , LTC6945.h
- get_LTC6946_global_fref_Hz() : LTC6946.cpp , LTC6946.h
- get_LTC6946_global_fref_MHz() : LTC6946.cpp , LTC6946.h
- get_LTC6946_global_frf_Hz() : LTC6946.cpp , LTC6946.h
- get_LTC6946_global_frf_MHz() : LTC6946.cpp , LTC6946.h
- get_LTC6946_REGSIZE() : LTC6946.cpp , LTC6946.h
- get_LTC6946_SPI_FIELD() : LTC6946.cpp , LTC6946.h
- get_LTC6946_SPI_FIELD_NUMBITS() : LTC6946.cpp , LTC6946.h
- get_LTC6946_SPI_FIELD_RW() : LTC6946.cpp , LTC6946.h
- get_LTC6947_global_fref_Hz() : LTC6947.cpp , LTC6947.h
- get_LTC6947_global_fref_MHz() : LTC6947.cpp , LTC6947.h
- get_LTC6947_global_frf_Hz() : LTC6947.cpp , LTC6947.h
- get_LTC6947_global_frf_MHz() : LTC6947.cpp , LTC6947.h
- get_LTC6947_global_VCO_MAX_Hz() : LTC6947.cpp , LTC6947.h
- get_LTC6947_global_VCO_MAX_MHz() : LTC6947.cpp , LTC6947.h
- get_LTC6947_global_VCO_MIN_Hz() : LTC6947.cpp , LTC6947.h
- get_LTC6947_global_VCO_MIN_MHz() : LTC6947.cpp , LTC6947.h
- get_LTC6947_REGSIZE() : LTC6947.cpp , LTC6947.h
- get_LTC6947_SPI_FIELD() : LTC6947.cpp , LTC6947.h
- get_LTC6947_SPI_FIELD_NUMBITS() : LTC6947.cpp , LTC6947.h
- get_LTC6947_SPI_FIELD_RW() : LTC6947.cpp , LTC6947.h
- get_LTC6948_global_fref_Hz() : LTC6948.cpp , LTC6948.h
- get_LTC6948_global_fref_MHz() : LTC6948.cpp , LTC6948.h
- get_LTC6948_global_frf_Hz() : LTC6948.cpp , LTC6948.h
- get_LTC6948_global_frf_MHz() : LTC6948.cpp , LTC6948.h
- get_LTC6948_REGSIZE() : LTC6948.cpp , LTC6948.h
- get_LTC6948_SPI_FIELD() : LTC6948.cpp , LTC6948.h
- get_LTC6948_SPI_FIELD_NUMBITS() : LTC6948.cpp , LTC6948.h
- get_LTC6948_SPI_FIELD_RW() : LTC6948.cpp , LTC6948.h
- get_LTC6950_global_fref_Hz() : LTC6950.cpp , LTC6950.h
- get_LTC6950_global_fref_MHz() : LTC6950.cpp , LTC6950.h
- get_LTC6950_global_frf_Hz() : LTC6950.cpp , LTC6950.h
- get_LTC6950_global_frf_MHz() : LTC6950.cpp , LTC6950.h
- get_LTC6950_global_VCO_MAX_Hz() : LTC6950.cpp , LTC6950.h
- get_LTC6950_global_VCO_MAX_MHz() : LTC6950.cpp , LTC6950.h
- get_LTC6950_global_VCO_MIN_Hz() : LTC6950.cpp , LTC6950.h
- get_LTC6950_global_VCO_MIN_MHz() : LTC6950.cpp , LTC6950.h
- get_LTC6950_REGSIZE() : LTC6950.cpp , LTC6950.h
- get_LTC6950_SPI_FIELD() : LTC6950.cpp , LTC6950.h
- get_LTC6950_SPI_FIELD_NUMBITS() : LTC6950.cpp , LTC6950.h
- get_LTC6950_SPI_FIELD_RW() : LTC6950.cpp , LTC6950.h
- get_LTC6951_REGSIZE() : LTC6951.h , LTC6951.cpp
- get_LTC6951_SPI_FIELD() : LTC6951.cpp , LTC6951.h
- get_LTC6951_SPI_FIELD_NUMBITS() : LTC6951.cpp , LTC6951.h
- get_LTC6951_SPI_FIELD_RW() : LTC6951.cpp , LTC6951.h
- get_LTC6952_REGSIZE() : LTC6952.cpp , LTC6952.h
- get_LTC6952_SPI_FIELD() : LTC6952.cpp , LTC6952.h
- get_LTC6952_SPI_FIELD_NUMBITS() : LTC6952.cpp , LTC6952.h
- get_LTC6952_SPI_FIELD_RW() : LTC6952.cpp , LTC6952.h
- get_LTC6953_REGSIZE() : LTC6953.cpp , LTC6953.h
- get_LTC6953_SPI_FIELD() : LTC6953.cpp , LTC6953.h
- get_LTC6953_SPI_FIELD_NUMBITS() : LTC6953.cpp , LTC6953.h
- get_LTC6953_SPI_FIELD_RW() : LTC6953.cpp , LTC6953.h
- get_LTC6954_REGSIZE() : LTC6954.cpp , LTC6954.h
- get_LTC6954_SPI_FIELD() : LTC6954.cpp , LTC6954.h
- get_LTC6954_SPI_FIELD_NUMBITS() : LTC6954.cpp , LTC6954.h
- get_LTC6954_SPI_FIELD_RW() : LTC6954.cpp , LTC6954.h
- get_mask() : LTC4155.c
- get_offset() : LTC4155.c
- get_record() : nvm.cpp
- get_record_data() : nvm.cpp
- get_result() : support_functions_LTC2986.h , support_functions_LTC2983.cpp , support_functions_LTC2983.h , support_functions_LTC2984.cpp , support_functions_LTC2984.h , support_functions_LTC2986.cpp
- get_size() : LTC4155.c
- get_start_address() : support_functions_LTC2984.h , support_functions_LTC2986.h , support_functions_LTC2986.cpp , support_functions_LTC2983.cpp , support_functions_LTC2983.h , support_functions_LTC2984.cpp
- get_subaddr() : LTC4155.c
- get_voltage() : DC2197.ino , DC2196A.ino , DC2376A.ino , DC1529A.ino , DC1534A.ino , DC1333A.ino , DC579A.ino , DC809A.ino , DC935A.ino , DC1466.ino , DC1096B.ino , DC1678A.ino , DC1397A.ino , DC2025A.ino , DC934A.ino , DC1333A.ino , DC1703A.ino
- get_voltage_code() : EVAL-AD5686R.ino , EVAL-AD5696R.ino
- get_voltage_float() : EVAL-AD5686R.ino , EVAL-AD5696R.ino
- getIGain() : LTC6115.h , LTC6115.cpp
- getMaxRecordSize() : nvm_data_helpers.cpp , nvm_data_helpers.h
- getRecordData() : nvm_data_helpers.h , nvm_data_helpers.cpp
- getRecordHoldData() : nvm_data_helpers.h , nvm_data_helpers.cpp
- getToken() : EasySMU_Run.ino
- getVGain() : LTC6115.h , LTC6115.cpp
- global_config_data : DC2222AB.ino , DC2222_interrupt_driven_read.ino , DC2222AC.ino
- globaltime_ms : DC2839A.ino
- gm : DC2155A.ino
- gm_dec : DC2155A.ino
- gm_decimal2hex() : DC2155A.ino
- gm_hex2decimal() : DC2155A.ino
- GM_MAX : DC2155A.ino
- gm_nearest_legal_value() : DC2155A.ino
- gm_vals : DC2155A.ino
- gm_vals_hex : DC2155A.ino
- go_idle_cfg_tbctl() : DC2334A.ino
- gpio_direction_input() : platform_drivers.cpp , platform_drivers.h
- gpio_direction_output() : platform_drivers.h , platform_drivers.cpp
- gpio_gain : EVAL-AD5686R.ino , EVAL-AD5696R.ino
- gpio_get() : platform_drivers.cpp , platform_drivers.h
- gpio_get_direction() : platform_drivers.h , platform_drivers.cpp
- gpio_get_value() : platform_drivers.cpp , platform_drivers.h
- GPIO_HIGH : platform_drivers.h
- GPIO_IN : platform_drivers.h
- GPIO_LOW : platform_drivers.h
- GPIO_OUT : platform_drivers.h
- gpio_remove() : platform_drivers.cpp , platform_drivers.h
- gpio_set_value() : platform_drivers.h , platform_drivers.cpp
- gpio_settings : DC1304A_B.ino , DC1304A_A.ino
- gpio_type : platform_drivers.h
- GPIOBITS : DC2515.ino
- GPIOBITS_A : DC2259.ino , DC2350AB.ino , DC2350AA.ino
- GPIOBITS_B : DC2350AB.ino , DC2350AA.ino
- GraphicUI() : DC2218A.ino
- greenBtn() : onoffbutton_breakout.ino , onoffbutton.ino
- GREENBUTTON_H : onoffbutton.ino , onoffbutton_breakout.ino
- GREENBUTTON_W : onoffbutton.ino , onoffbutton_breakout.ino
- GREENBUTTON_X : onoffbutton.ino , onoffbutton_breakout.ino
- GREENBUTTON_Y : onoffbutton.ino , onoffbutton_breakout.ino