| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
REG0
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

REG0 Register. More...

## Macros
#define | LTC4155_REG0_SUBADDR 0x00
#define | LTC4155_REG0 (0 << 12 | (16 - 1) << 8 | LTC4155_REG0_SUBADDR)

## Detailed Description

REG0 Register.

7 | 6 | 5 | 4:0
--- | --- | --- | ---
DISABLE_INPUT_UVCL | EN_BAT_CONDITIONER | LOCKOUT_ID_PIN | USBILIM

- CommandCode: 0x00
- Contains Bit Fields:
  - DISABLE_INPUT_UVCL : Disables automatic power reduction in response to low input voltage.
  - EN_BAT_CONDITIONER : Enables autonomous Overtemperature Battery Conditioner Load when the thermistor temperature exceeds 60°C.
  - LOCKOUT_ID_PIN : Disables autonomous USB OTG operation when the ID pin is grounded by an appropriate USB cable.
  - USBILIM : USB total input current limit setting. Register contents will be modified by the LTC4155 upon certain events. See the datasheet section Input Current Regulation.

## Macro Definition Documentation

## ◆ LTC4155_REG0

#define LTC4155_REG0 (0 << 12 | (16 - 1) << 8 | LTC4155_REG0_SUBADDR)

Definition at line 96 of file LTC4155_reg_defs.h.

## ◆ LTC4155_REG0_SUBADDR

#define LTC4155_REG0_SUBADDR 0x00

Definition at line 95 of file LTC4155_reg_defs.h.