| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Public Member Functions | Data Fields
LT_2977FaultLog::FaultLogLtc2977 Struct Reference

## Detailed Description

Definition at line 181 of file LT_2977FaultLog.h.

## Public Member Functions
bool | isValidData (void *pos, uint8_t size=2)

## Data Fields
struct FaultLogPreambleLtc2977 | preamble
uint8_t | telemetryData [208]
struct FaultLogReadLoopLtc2977 * | loops
uint8_t | firstValidByte
uint8_t | lastValidByte

## Member Function Documentation

## ◆ isValidData()

bool LT_2977FaultLog::FaultLogLtc2977::isValidData | ( | void * | pos,
|  | uint8_t | size = `2`
| ) |  |

Definition at line 72 of file LT_2977FaultLog.cpp.

## Field Documentation

## ◆ firstValidByte

uint8_t LT_2977FaultLog::FaultLogLtc2977::firstValidByte

Definition at line 187 of file LT_2977FaultLog.h.

## ◆ lastValidByte

uint8_t LT_2977FaultLog::FaultLogLtc2977::lastValidByte

Definition at line 188 of file LT_2977FaultLog.h.

## ◆ loops

struct FaultLogReadLoopLtc2977* LT_2977FaultLog::FaultLogLtc2977::loops

Definition at line 186 of file LT_2977FaultLog.h.

## ◆ preamble

struct FaultLogPreambleLtc2977 LT_2977FaultLog::FaultLogLtc2977::preamble

Definition at line 184 of file LT_2977FaultLog.h.

## ◆ telemetryData

uint8_t LT_2977FaultLog::FaultLogLtc2977::telemetryData[208]

Definition at line 185 of file LT_2977FaultLog.h.

The documentation for this struct was generated from the following files:

- LT_2977FaultLog.h
- LT_2977FaultLog.cpp