| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
DISABLE_INPUT_UVCL
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

DISABLE_INPUT_UVCL Bit Field. More...

## Macros
#define | LTC4155_DISABLE_INPUT_UVCL_SUBADDR LTC4155_REG0_SUBADDR
| DISABLE_INPUT_UVCL More...
#define | LTC4155_DISABLE_INPUT_UVCL_SIZE 1
#define | LTC4155_DISABLE_INPUT_UVCL_OFFSET 7
#define | LTC4155_DISABLE_INPUT_UVCL_MASK 0x80
#define | LTC4155_DISABLE_INPUT_UVCL (LTC4155_DISABLE_INPUT_UVCL_OFFSET << 12 | (LTC4155_DISABLE_INPUT_UVCL_SIZE - 1) << 8 | LTC4155_DISABLE_INPUT_UVCL_SUBADDR)

## Detailed Description

DISABLE_INPUT_UVCL Bit Field.

Disables automatic power reduction in response to low input voltage.

- Register: REG0
- CommandCode: 0x00
- Size: 1
- Offset: 7
- MSB: 7
- MASK: 0x80
- Access: R/W
- Default: 0

## Macro Definition Documentation

## ◆ LTC4155_DISABLE_INPUT_UVCL

#define LTC4155_DISABLE_INPUT_UVCL (LTC4155_DISABLE_INPUT_UVCL_OFFSET << 12 | (LTC4155_DISABLE_INPUT_UVCL_SIZE - 1) << 8 | LTC4155_DISABLE_INPUT_UVCL_SUBADDR)

Definition at line 117 of file LTC4155_reg_defs.h.

## ◆ LTC4155_DISABLE_INPUT_UVCL_MASK

#define LTC4155_DISABLE_INPUT_UVCL_MASK 0x80

Definition at line 116 of file LTC4155_reg_defs.h.

## ◆ LTC4155_DISABLE_INPUT_UVCL_OFFSET

#define LTC4155_DISABLE_INPUT_UVCL_OFFSET 7

Definition at line 115 of file LTC4155_reg_defs.h.

## ◆ LTC4155_DISABLE_INPUT_UVCL_SIZE

#define LTC4155_DISABLE_INPUT_UVCL_SIZE 1

Definition at line 114 of file LTC4155_reg_defs.h.

## ◆ LTC4155_DISABLE_INPUT_UVCL_SUBADDR

#define LTC4155_DISABLE_INPUT_UVCL_SUBADDR LTC4155_REG0_SUBADDR

DISABLE_INPUT_UVCL

Definition at line 113 of file LTC4155_reg_defs.h.