| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

### - s -

- sample : EVAL-AD7124-8.ino
- samples_counter : DC2839A.ino
- SCONV : DC2515.ino
- SDNb_val : DC2364A.ino
- SEL_ALL_REG : DC2350AB.ino , DC2515.ino , DC2259.ino , DC2350AA.ino
- SEL_REG_A : DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino
- SEL_REG_B : DC2350AB.ino , DC2515.ino , DC2259.ino , DC2350AA.ino
- SELECT : Precision_Voltage_Source.ino , Synth.ino
- sense_resistor : LTM9100.h , DC2423A.ino
- serial_data : EasySMU_Run.ino
- serial_mode : DC590_subset.ino , DC2430A.ino , DC590B.ino , DC590B_enhanced.ino
- servo0_value_hi : DC2467.ino
- servo0_value_low : DC2467.ino
- servo0_value_marg : DC980.ino
- servo0_value_nom : DC2467.ino , DC980.ino
- servo1_value_hi : DC2467.ino
- servo1_value_low : DC2467.ino
- servo1_value_marg : DC980.ino
- servo1_value_nom : DC2467.ino , DC980.ino
- set : DC2218A.ino
- setpoint : LT1054_voltage_mode_buck.ino , LT1054_voltage_mode_buck_DC_ctrl.ino
- shdn_settings : DC1304A_A.ino , DC1304A_B.ino
- shift_count : DC579A.ino , DC809A.ino , DC935A.ino , DC1466.ino , DC1534A.ino , DC1333A.ino , DC1678A.ino , DC1703A.ino , DC1397A.ino , DC1529A.ino
- sign : Precision_Voltage_Source.ino
- SINGLE_ENDED_CONFIG_ARRAY : LTC2449_Datalogger.ino , LTC24XX_general_test.ino
- single_ended_differential : DC682A.ino , DC1444A.ino , DC1186A.ino , DC1337A.ino
- smbus : DC1674A.ino , DC2675A.ino , DC1978.ino , Part Number/2000/2900/2974/faultlog/faultlog.ino , DC2022A.ino , DC2382.ino , Part Number/2000/2900/2975/faultlog/faultlog.ino , DC2028A.ino , DC1936A.ino , Part Number/2000/2900/2977/faultlog/faultlog.ino , Part Number/2000/2900/2978/faultlog/faultlog.ino , DC2198A.ino , Part Number/2000/2900/2980/faultlog/faultlog.ino , DC2023A.ino , Part Number/2000/2900/2987/faultlog/faultlog.ino , DC1590B.ino , Part Number/3000/3800/3880/faultlog/faultlog.ino , Part Number/3000/3800/3882/faultlog/faultlog.ino , DC1778A.ino , Part Number/3000/3800/3883/faultlog/faultlog.ino , DC2155A.ino , DC2263A.ino , fast_telemetry.ino , Part Number/3000/3800/3887/faultlog/faultlog.ino , DC2875A.ino , DC1811B.ino , DC1989A.ino , DC2978A.ino , hello_world.ino , program.ino , retention.ino , User Contributed/DC1962C/faultlog/faultlog.ino , ultra_fix.ino , sandbox.ino , svid.ino , DC1633B.ino , DC1605B.ino , DC2313A.ino , DC2467.ino , DC980.ino
- smbusNoPec : program.ino , device_logger.ino , rail_logger.ino , svid.ino
- smbusNoPec__ : nvm_data_helpers.h , nvm.cpp , main_record_processor.h , nvm.h
- smbusPec : program.ino , svid.ino , rail_logger.ino , device_logger.ino
- smbusPec__ : nvm.cpp , main_record_processor.h , nvm_data_helpers.h , nvm.h
- smoothing_const : DC1410AB.ino , DC1410AA.ino
- SMU : EasySMU_Run.ino
- spi_divider : DC2430A.ino , DC590B_enhanced.ino , DC590B.ino
- spi_mode : DC590B.ino , DC2430A.ino , DC590B_enhanced.ino , DC590_subset.ino
- spi_out : DC1304A_B.ino , DC1304A_A.ino
- spi_params : EVAL-AD7124-8.ino , EVAL-AD5686R.ino , EVAL-AD5696R.ino
- start : Audio_Spectrum_Analyzer.ino
- start_millis : DC2839A.ino
- startMinutes : vmClock.ino
- startsequence : DC2218A.ino
- startup : DC2218A.ino
- STAT_CH_TO_CONVERT : DC2350AA.ino , DC2350AB.ino , DC2515.ino , DC2259.ino
- state : LT1054_voltage_mode_buck_DC_ctrl.ino
- statusRegs : DC2574A_KIT.ino
- statusRegsRead : DC2574A_KIT.ino
- step : Audio_Spectrum_Analyzer.ino
- stimulus : DC2741_production_test.ino
- stop : Audio_Spectrum_Analyzer.ino