| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Data Structures | Data Fields
EasySMU::eeprom_data_union Union Reference

Union that defines the calibration data stored in the EasySMU EEPROM. More...

## Detailed Description

Union that defines the calibration data stored in the EasySMU EEPROM.

Definition at line 290 of file EasySMU.h.

## Data Structures
struct | data_struct_type
| This struct holds all of the calibration data, i.e. offset integers, LSB floats, etc. The eeprom_data_union contains a byte_array that is used to write and read this data to/from the EEPROM. More...

## Data Fields
struct EasySMU::eeprom_data_union::data_struct_type | calibration
char | byte_array [sizeof(data_struct_type)]

## Field Documentation

## ◆ byte_array

char EasySMU::eeprom_data_union::byte_array[sizeof(data_struct_type)]

Definition at line 314 of file EasySMU.h.

## ◆ calibration

struct EasySMU::eeprom_data_union::data_struct_type EasySMU::eeprom_data_union::calibration

The documentation for this union was generated from the following file:

- EasySMU.h