| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
BAD_CELL
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

BAD_CELL Bit Field. More...

## Macros
#define | LTC4155_BAD_CELL_SUBADDR LTC4155_REG4_SUBADDR
| BAD_CELL More...
#define | LTC4155_BAD_CELL_SIZE 1
#define | LTC4155_BAD_CELL_OFFSET 0
#define | LTC4155_BAD_CELL_MASK 0x01
#define | LTC4155_BAD_CELL (LTC4155_BAD_CELL_OFFSET << 12 | (LTC4155_BAD_CELL_SIZE - 1) << 8 | LTC4155_BAD_CELL_SUBADDR)

## Detailed Description

BAD_CELL Bit Field.

Battery unresponsive to charging for 30 minutes.

- Register: REG4
- CommandCode: 0x04
- Size: 1
- Offset: 0
- MSB: 0
- MASK: 0x01
- Access: R
- Default: n/a

## Macro Definition Documentation

## ◆ LTC4155_BAD_CELL

#define LTC4155_BAD_CELL (LTC4155_BAD_CELL_OFFSET << 12 | (LTC4155_BAD_CELL_SIZE - 1) << 8 | LTC4155_BAD_CELL_SUBADDR)

Definition at line 742 of file LTC4155_reg_defs.h.

## ◆ LTC4155_BAD_CELL_MASK

#define LTC4155_BAD_CELL_MASK 0x01

Definition at line 741 of file LTC4155_reg_defs.h.

## ◆ LTC4155_BAD_CELL_OFFSET

#define LTC4155_BAD_CELL_OFFSET 0

Definition at line 740 of file LTC4155_reg_defs.h.

## ◆ LTC4155_BAD_CELL_SIZE

#define LTC4155_BAD_CELL_SIZE 1

Definition at line 739 of file LTC4155_reg_defs.h.

## ◆ LTC4155_BAD_CELL_SUBADDR

#define LTC4155_BAD_CELL_SUBADDR LTC4155_REG4_SUBADDR

BAD_CELL

Definition at line 738 of file LTC4155_reg_defs.h.