| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
ENABLE_CHARGER_INT
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

ENABLE_CHARGER_INT Bit Field. More...

## Macros
#define | LTC4155_ENABLE_CHARGER_INT_SUBADDR LTC4155_REG6_SUBADDR
| ENABLE_CHARGER_INT More...
#define | LTC4155_ENABLE_CHARGER_INT_SIZE 1
#define | LTC4155_ENABLE_CHARGER_INT_OFFSET 7
#define | LTC4155_ENABLE_CHARGER_INT_MASK 0x80
#define | LTC4155_ENABLE_CHARGER_INT (LTC4155_ENABLE_CHARGER_INT_OFFSET << 12 | (LTC4155_ENABLE_CHARGER_INT_SIZE - 1) << 8 | LTC4155_ENABLE_CHARGER_INT_SUBADDR)

## Detailed Description

ENABLE_CHARGER_INT Bit Field.

Enable battery CHARGER_STATUS interrupts.

- Register: REG6
- CommandCode: 0x06
- Size: 1
- Offset: 7
- MSB: 7
- MASK: 0x80
- Access: R/W
- Default: 0

## Macro Definition Documentation

## ◆ LTC4155_ENABLE_CHARGER_INT

#define LTC4155_ENABLE_CHARGER_INT (LTC4155_ENABLE_CHARGER_INT_OFFSET << 12 | (LTC4155_ENABLE_CHARGER_INT_SIZE - 1) << 8 | LTC4155_ENABLE_CHARGER_INT_SUBADDR)

Definition at line 850 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_CHARGER_INT_MASK

#define LTC4155_ENABLE_CHARGER_INT_MASK 0x80

Definition at line 849 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_CHARGER_INT_OFFSET

#define LTC4155_ENABLE_CHARGER_INT_OFFSET 7

Definition at line 848 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_CHARGER_INT_SIZE

#define LTC4155_ENABLE_CHARGER_INT_SIZE 1

Definition at line 847 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_CHARGER_INT_SUBADDR

#define LTC4155_ENABLE_CHARGER_INT_SUBADDR LTC4155_REG6_SUBADDR

ENABLE_CHARGER_INT

Definition at line 846 of file LTC4155_reg_defs.h.