| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
OTG_FAULT
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

OTG_FAULT Bit Field. More...

## Macros
#define | LTC4155_OTG_FAULT_SUBADDR LTC4155_REG4_SUBADDR
| OTG_FAULT More...
#define | LTC4155_OTG_FAULT_SIZE 1
#define | LTC4155_OTG_FAULT_OFFSET 1
#define | LTC4155_OTG_FAULT_MASK 0x02
#define | LTC4155_OTG_FAULT (LTC4155_OTG_FAULT_OFFSET << 12 | (LTC4155_OTG_FAULT_SIZE - 1) << 8 | LTC4155_OTG_FAULT_SUBADDR)

## Detailed Description

OTG_FAULT Bit Field.

USB On-The-Go step-up regulator fault shutdown.

- Register: REG4
- CommandCode: 0x04
- Size: 1
- Offset: 1
- MSB: 1
- MASK: 0x02
- Access: R
- Default: n/a

## Macro Definition Documentation

## ◆ LTC4155_OTG_FAULT

#define LTC4155_OTG_FAULT (LTC4155_OTG_FAULT_OFFSET << 12 | (LTC4155_OTG_FAULT_SIZE - 1) << 8 | LTC4155_OTG_FAULT_SUBADDR)

Definition at line 721 of file LTC4155_reg_defs.h.

## ◆ LTC4155_OTG_FAULT_MASK

#define LTC4155_OTG_FAULT_MASK 0x02

Definition at line 720 of file LTC4155_reg_defs.h.

## ◆ LTC4155_OTG_FAULT_OFFSET

#define LTC4155_OTG_FAULT_OFFSET 1

Definition at line 719 of file LTC4155_reg_defs.h.

## ◆ LTC4155_OTG_FAULT_SIZE

#define LTC4155_OTG_FAULT_SIZE 1

Definition at line 718 of file LTC4155_reg_defs.h.

## ◆ LTC4155_OTG_FAULT_SUBADDR

#define LTC4155_OTG_FAULT_SUBADDR LTC4155_REG4_SUBADDR

OTG_FAULT

Definition at line 717 of file LTC4155_reg_defs.h.