| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
NTCVAL
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

NTCVAL Bit Field. More...

## Macros
#define | LTC4155_NTCVAL_SUBADDR LTC4155_REG5_SUBADDR
| NTCVAL More...
#define | LTC4155_NTCVAL_SIZE 7
#define | LTC4155_NTCVAL_OFFSET 1
#define | LTC4155_NTCVAL_MASK 0xFE
#define | LTC4155_NTCVAL (LTC4155_NTCVAL_OFFSET << 12 | (LTC4155_NTCVAL_SIZE - 1) << 8 | LTC4155_NTCVAL_SUBADDR)

## Detailed Description

NTCVAL Bit Field.

NTC pin (thermistor) ADC conversion result.

- Register: REG5
- CommandCode: 0x05
- Size: 7
- Offset: 1
- MSB: 7
- MASK: 0xFE
- Access: R
- Default: n/a

## Macro Definition Documentation

## ◆ LTC4155_NTCVAL

#define LTC4155_NTCVAL (LTC4155_NTCVAL_OFFSET << 12 | (LTC4155_NTCVAL_SIZE - 1) << 8 | LTC4155_NTCVAL_SUBADDR)

Definition at line 782 of file LTC4155_reg_defs.h.

## ◆ LTC4155_NTCVAL_MASK

#define LTC4155_NTCVAL_MASK 0xFE

Definition at line 781 of file LTC4155_reg_defs.h.

## ◆ LTC4155_NTCVAL_OFFSET

#define LTC4155_NTCVAL_OFFSET 1

Definition at line 780 of file LTC4155_reg_defs.h.

## ◆ LTC4155_NTCVAL_SIZE

#define LTC4155_NTCVAL_SIZE 7

Definition at line 779 of file LTC4155_reg_defs.h.

## ◆ LTC4155_NTCVAL_SUBADDR

#define LTC4155_NTCVAL_SUBADDR LTC4155_REG5_SUBADDR

NTCVAL

Definition at line 778 of file LTC4155_reg_defs.h.