| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
REG6
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

REG6 Register. More...

## Macros
#define | LTC4155_REG6_SUBADDR 0x06
#define | LTC4155_REG6 (0 << 12 | (16 - 1) << 8 | LTC4155_REG6_SUBADDR)

## Detailed Description

REG6 Register.

7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | ---
ENABLE_CHARGER_INT | ENABLE_FAULT_INT | ENABLE_EXTPWR_INT | ENABLE_OTG_INT | ENABLE_AT_ILIM_INT | ENABLE_INPUT_UVCL_INT | REQUEST_OTG | RESERVED

Interrupt Mask Resister

- CommandCode: 0x06
- Contains Bit Fields:
  - ENABLE_CHARGER_INT : Enable battery CHARGER_STATUS interrupts.
  - ENABLE_FAULT_INT : Enable OVP_ACTIVE, OTG_FAULT, BAD_CELL, and NTCSTAT = Hot_Fault interrupts.
  - ENABLE_EXTPWR_INT : Enable USBSNS_GOOD, WALLSNS_GOOD, EXT_PWR_GOOD external power available interrupts.
  - ENABLE_OTG_INT : Enable ID_PIN_DETECT and OTG_ENABLED USB On-The-Go interrupts.
  - ENABLE_AT_ILIM_INT : Enable AT_INPUT_ILIM interrupts.
  - ENABLE_INPUT_UVCL_INT : Enable INPUT_UVCL_ACTIVE interrupts.
  - REQUEST_OTG : USB On-The-Go step-up voltage converter manual activation setting.
  - RESERVED : Always set to 0.

## Macro Definition Documentation

## ◆ LTC4155_REG6

#define LTC4155_REG6 (0 << 12 | (16 - 1) << 8 | LTC4155_REG6_SUBADDR)

Definition at line 829 of file LTC4155_reg_defs.h.

## ◆ LTC4155_REG6_SUBADDR

#define LTC4155_REG6_SUBADDR 0x06

Definition at line 828 of file LTC4155_reg_defs.h.