| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
REG5
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

REG5 Register. More...

## Macros
#define | LTC4155_REG5_SUBADDR 0x05
#define | LTC4155_REG5 (0 << 12 | (16 - 1) << 8 | LTC4155_REG5_SUBADDR)

## Detailed Description

REG5 Register.

7:1 | 0
--- | ---
NTCVAL | NTC_WARNING

- CommandCode: 0x05
- Contains Bit Fields:
  - NTCVAL : NTC pin (thermistor) ADC conversion result.
  - NTC_WARNING : Thermistor temperature out of range for battery charging.

## Macro Definition Documentation

## ◆ LTC4155_REG5

#define LTC4155_REG5 (0 << 12 | (16 - 1) << 8 | LTC4155_REG5_SUBADDR)

Definition at line 761 of file LTC4155_reg_defs.h.

## ◆ LTC4155_REG5_SUBADDR

#define LTC4155_REG5_SUBADDR 0x05

Definition at line 760 of file LTC4155_reg_defs.h.