| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
REG7
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

REG7 Register. More...

## Macros
#define | LTC4155_REG7_SUBADDR 0x07
#define | LTC4155_REG7 (0 << 12 | (16 - 1) << 8 | LTC4155_REG7_SUBADDR)

## Detailed Description

REG7 Register.

7:0
ARM_SHIPMODE

- CommandCode: 0x07
- Contains Bit Fields:
  - ARM_SHIPMODE : Write any data to this address to enable ship-and-store shutdown mode

## Macro Definition Documentation

## ◆ LTC4155_REG7

#define LTC4155_REG7 (0 << 12 | (16 - 1) << 8 | LTC4155_REG7_SUBADDR)

Definition at line 1015 of file LTC4155_reg_defs.h.

## ◆ LTC4155_REG7_SUBADDR

#define LTC4155_REG7_SUBADDR 0x07

Definition at line 1014 of file LTC4155_reg_defs.h.