| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
PRIORITY
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

PRIORITY Bit Field. More...

## Macros
#define | LTC4155_PRIORITY_SUBADDR LTC4155_REG1_SUBADDR
| PRIORITY More...
#define | LTC4155_PRIORITY_SIZE 1
#define | LTC4155_PRIORITY_OFFSET 7
#define | LTC4155_PRIORITY_MASK 0x80
#define | LTC4155_PRIORITY (LTC4155_PRIORITY_OFFSET << 12 | (LTC4155_PRIORITY_SIZE - 1) << 8 | LTC4155_PRIORITY_SUBADDR)
#define | LTC4155_PRIORITY_PRESET_WALL 0x0
#define | LTC4155_PRIORITY_PRESET_USB 0x1

## Detailed Description

PRIORITY Bit Field.

Input connector priority swap setting. Setting PRIORITY will cause power to be drawn from USB when both WALL and USB power are present.

- Register: REG1
- CommandCode: 0x01
- Size: 1
- Offset: 7
- MSB: 7
- MASK: 0x80
- Access: R/W
- Default: 0

## Macro Definition Documentation

## ◆ LTC4155_PRIORITY

#define LTC4155_PRIORITY (LTC4155_PRIORITY_OFFSET << 12 | (LTC4155_PRIORITY_SIZE - 1) << 8 | LTC4155_PRIORITY_SUBADDR)

Definition at line 238 of file LTC4155_reg_defs.h.

## ◆ LTC4155_PRIORITY_MASK

#define LTC4155_PRIORITY_MASK 0x80

Definition at line 237 of file LTC4155_reg_defs.h.

## ◆ LTC4155_PRIORITY_OFFSET

#define LTC4155_PRIORITY_OFFSET 7

Definition at line 236 of file LTC4155_reg_defs.h.

## ◆ LTC4155_PRIORITY_PRESET_USB

#define LTC4155_PRIORITY_PRESET_USB 0x1

Definition at line 240 of file LTC4155_reg_defs.h.

## ◆ LTC4155_PRIORITY_PRESET_WALL

#define LTC4155_PRIORITY_PRESET_WALL 0x0

Definition at line 239 of file LTC4155_reg_defs.h.

## ◆ LTC4155_PRIORITY_SIZE

#define LTC4155_PRIORITY_SIZE 1

Definition at line 235 of file LTC4155_reg_defs.h.

## ◆ LTC4155_PRIORITY_SUBADDR

#define LTC4155_PRIORITY_SUBADDR LTC4155_REG1_SUBADDR

PRIORITY

Definition at line 234 of file LTC4155_reg_defs.h.