| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
RESERVED
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

RESERVED Bit Field. More...

## Macros
#define | LTC4155_RESERVED_SUBADDR LTC4155_REG6_SUBADDR
| RESERVED More...
#define | LTC4155_RESERVED_SIZE 1
#define | LTC4155_RESERVED_OFFSET 0
#define | LTC4155_RESERVED_MASK 0x01
#define | LTC4155_RESERVED (LTC4155_RESERVED_OFFSET << 12 | (LTC4155_RESERVED_SIZE - 1) << 8 | LTC4155_RESERVED_SUBADDR)

## Detailed Description

RESERVED Bit Field.

Always set to 0.

- Register: REG6
- CommandCode: 0x06
- Size: 1
- Offset: 0
- MSB: 0
- MASK: 0x01
- Access: R/W
- Default: 0

## Macro Definition Documentation

## ◆ LTC4155_RESERVED

#define LTC4155_RESERVED (LTC4155_RESERVED_OFFSET << 12 | (LTC4155_RESERVED_SIZE - 1) << 8 | LTC4155_RESERVED_SUBADDR)

Definition at line 997 of file LTC4155_reg_defs.h.

## ◆ LTC4155_RESERVED_MASK

#define LTC4155_RESERVED_MASK 0x01

Definition at line 996 of file LTC4155_reg_defs.h.

## ◆ LTC4155_RESERVED_OFFSET

#define LTC4155_RESERVED_OFFSET 0

Definition at line 995 of file LTC4155_reg_defs.h.

## ◆ LTC4155_RESERVED_SIZE

#define LTC4155_RESERVED_SIZE 1

Definition at line 994 of file LTC4155_reg_defs.h.

## ◆ LTC4155_RESERVED_SUBADDR

#define LTC4155_RESERVED_SUBADDR LTC4155_REG6_SUBADDR

RESERVED

Definition at line 993 of file LTC4155_reg_defs.h.