| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
EasySMU.cpp File Reference
Example Designs » EasySMU: I2C Address Translator Demonstration and a Simple Multi-Channel Source Measurement Unit

EasySMU Class: I2C Address Translator Demonstration and a Simple Multi-Channel Source Measurement Unit. More...

## Detailed Description

EasySMU Class: I2C Address Translator Demonstration and a Simple Multi-Channel Source Measurement Unit.

Definition in file EasySMU.cpp.

Go to the source code of this file.

## Macros
#define | LTC2485_TIMEOUT (_LTC2485_CONVERSION_TIME)
| Maximum time allowed for LTC2485 conversion. If this time is exceeded, something is wrong. More...
#define | float_current_source_setting_equation(Idac_pullup_code, current_source_pullup_offset, current_source_pullup_LSB) (((int32_t)Idac_pullup_code_ + (int32_t)current_source_pullup_offset) * current_source_pullup_LSB)

## Macro Definition Documentation

## ◆ float_current_source_setting_equation

#define float_current_source_setting_equation | ( |  | Idac_pullup_code,
|  |  | current_source_pullup_offset,
|  |  | current_source_pullup_LSB
| ) |  | (((int32_t)Idac_pullup_code_ + (int32_t)current_source_pullup_offset) * current_source_pullup_LSB)

Definition at line 134 of file EasySMU.cpp.

## ◆ LTC2485_TIMEOUT

#define LTC2485_TIMEOUT (_LTC2485_CONVERSION_TIME)

Maximum time allowed for LTC2485 conversion. If this time is exceeded, something is wrong.

Definition at line 68 of file EasySMU.cpp.