| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
AT_INPUT_ILIM
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

AT_INPUT_ILIM Bit Field. More...

## Macros
#define | LTC4155_AT_INPUT_ILIM_SUBADDR LTC4155_REG4_SUBADDR
| AT_INPUT_ILIM More...
#define | LTC4155_AT_INPUT_ILIM_SIZE 1
#define | LTC4155_AT_INPUT_ILIM_OFFSET 4
#define | LTC4155_AT_INPUT_ILIM_MASK 0x10
#define | LTC4155_AT_INPUT_ILIM (LTC4155_AT_INPUT_ILIM_OFFSET << 12 | (LTC4155_AT_INPUT_ILIM_SIZE - 1) << 8 | LTC4155_AT_INPUT_ILIM_SUBADDR)

## Detailed Description

AT_INPUT_ILIM Bit Field.

Input current limit control circuit engaged.

- Register: REG4
- CommandCode: 0x04
- Size: 1
- Offset: 4
- MSB: 4
- MASK: 0x10
- Access: R
- Default: n/a

## Macro Definition Documentation

## ◆ LTC4155_AT_INPUT_ILIM

#define LTC4155_AT_INPUT_ILIM (LTC4155_AT_INPUT_ILIM_OFFSET << 12 | (LTC4155_AT_INPUT_ILIM_SIZE - 1) << 8 | LTC4155_AT_INPUT_ILIM_SUBADDR)

Definition at line 658 of file LTC4155_reg_defs.h.

## ◆ LTC4155_AT_INPUT_ILIM_MASK

#define LTC4155_AT_INPUT_ILIM_MASK 0x10

Definition at line 657 of file LTC4155_reg_defs.h.

## ◆ LTC4155_AT_INPUT_ILIM_OFFSET

#define LTC4155_AT_INPUT_ILIM_OFFSET 4

Definition at line 656 of file LTC4155_reg_defs.h.

## ◆ LTC4155_AT_INPUT_ILIM_SIZE

#define LTC4155_AT_INPUT_ILIM_SIZE 1

Definition at line 655 of file LTC4155_reg_defs.h.

## ◆ LTC4155_AT_INPUT_ILIM_SUBADDR

#define LTC4155_AT_INPUT_ILIM_SUBADDR LTC4155_REG4_SUBADDR

AT_INPUT_ILIM

Definition at line 654 of file LTC4155_reg_defs.h.