| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Functions | Variables
FAE_April_2013.ino File Reference
Digital-to-Analog Converters (DAC) » LTC2607: 16-Bit, Dual Rail-to-Rail DACs with I2C Interface

DC934A Science Project FAE Meeting April 2013. More...

## Detailed Description

DC934A Science Project FAE Meeting April 2013.

Definition in file FAE_April_2013.ino.

Go to the source code of this file.

## Functions
static void | setup ()
| Initialize Linduino once on power-up or reset. More...
static void | loop ()

## Variables
const uint16_t | LTC2422_timeout = 1000
| The timeout for the LTC2422. More...

## Function Documentation

## ◆ loop()

static void loop | ( | void |  | ) |
| static

Definition at line 98 of file FAE_April_2013.ino.

## ◆ setup()

static void setup | ( | void |  | ) |
| static

Initialize Linduino once on power-up or reset.

Definition at line 58 of file FAE_April_2013.ino.

## Variable Documentation

## ◆ LTC2422_timeout

const uint16_t LTC2422_timeout = 1000

The timeout for the LTC2422.

Definition at line 55 of file FAE_April_2013.ino.