| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - s -

- sample : EVAL-AD7124-8.ino
- samples_counter : DC2839A.ino
- SC_ADDR_0 : LT3965.h
- SCAN_MODE_DISPLAY_DELAY : DC1496BB.ino , DC1812AA.ino , DC1812A-B.ino
- SCONV : DC2515.ino
- SCREEN_UPDATE_TIME : DC2574A_KIT.ino
- SCREENSETCURSOR : LCDKeypad.h
- SCTL : DC2350AA.ino , DC2350AB.ino
- SD_CS : spitftbitmap.ino
- SDNb_val : DC2364A.ino
- sectionalBlanking() : DC2218A.ino
- SEL_ALL_REG : DC2259.ino , DC2350AA.ino , DC2350AB.ino , DC2515.ino
- SEL_REG_A : DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino
- SEL_REG_B : DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino
- SELECT : Precision_Voltage_Source.ino , Synth.ino
- select_s_pin() : DC2350AB.ino , DC2515.ino , DC2259.ino , DC2350AA.ino
- SELFTEST_1 : LTC681x.h
- SELFTEST_2 : LTC681x.h
- send_pulses() : LTC2508.cpp , LTC2508.h , LTC2512.cpp , LTC2512.h
- sense_resistor : LTM9100.h , DC2423A.ino
- SENSE_RESISTOR : DC874A.ino , DC786A.ino , DC1704A.ino
- SENSE_RESISTOR_VALUE_LSB : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_ABOVE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_BELOW : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_HARD_FAILURE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__ACTIVE_ANALOG : configuration_constants_LTC2986.h
- SENSOR_TYPE__CUSTOM_THERMOCOUPLE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__DIRECT_ADC : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__NONE : configuration_constants_LTC2984.h , configuration_constants_LTC2986.h , configuration_constants_LTC2983.h
- SENSOR_TYPE__OFF_CHIP_DIODE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__RTD_CUSTOM : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__RTD_NI_120 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__RTD_PT_10 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__RTD_PT_100 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__RTD_PT_1000 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__RTD_PT_1000_375 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__RTD_PT_200 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__RTD_PT_50 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__RTD_PT_500 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__SENSE_RESISTOR : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__THERMISTOR_1003K_1K_25C : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__THERMISTOR_44004_2P252K_25C : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__THERMISTOR_44005_3K_25C : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__THERMISTOR_44006_10K_25C : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__THERMISTOR_44007_5K_25C : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__THERMISTOR_44008_30K_25C : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__THERMISTOR_CUSTOM_STEINHART_HART : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__THERMISTOR_CUSTOM_TABLE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__THERMISTOR_YSI_400_2P252K_25C : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__TYPE_B_THERMOCOUPLE : configuration_constants_LTC2986.h , configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- SENSOR_TYPE__TYPE_E_THERMOCOUPLE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__TYPE_J_THERMOCOUPLE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__TYPE_K_THERMOCOUPLE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__TYPE_N_THERMOCOUPLE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__TYPE_R_THERMOCOUPLE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__TYPE_S_THERMOCOUPLE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE__TYPE_T_THERMOCOUPLE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- SENSOR_TYPE_LSB : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- sequence_off_on() : DC2875A.ino , DC2675A.ino , DC1978.ino , DC2022A.ino , DC2382.ino , DC2028A.ino , DC2198A.ino , DC2023A.ino , DC1590B.ino , DC1936A.ino , DC1778A.ino , DC2263A.ino , DC1811B.ino , hello_world.ino
- SERIAL_COMMANDS_ERROR : EasySMU_Run.ino
- SERIAL_COMMANDS_SIZE_0 : EasySMU_Run.ino
- SERIAL_COMMANDS_SIZE_1 : EasySMU_Run.ino
- SERIAL_COMMANDS_SIZE_12 : EasySMU_Run.ino
- SERIAL_COMMANDS_SIZE_121 : EasySMU_Run.ino
- SERIAL_COMMANDS_SIZE_122 : EasySMU_Run.ino
- SERIAL_COMMANDS_SIZE_LCD : EasySMU_Run.ino
- serial_data : EasySMU_Run.ino
- serial_mode : DC590_subset.ino , DC2430A.ino , DC590B.ino , DC590B_enhanced.ino
- serial_print_hex() : DC1651A.ino , DC1652A.ino , DC1894.ino , DC1942.ino , DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino
- serial_print_text() : DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino
- SERIAL_TERMINATOR : UserInterface.h
- servo0_value_hi : DC2467.ino
- servo0_value_low : DC2467.ino
- servo0_value_marg : DC980.ino
- servo0_value_nom : DC2467.ino , DC980.ino
- servo1_value_hi : DC2467.ino
- servo1_value_low : DC2467.ino
- servo1_value_marg : DC980.ino
- servo1_value_nom : DC2467.ino , DC980.ino
- set : DC2218A.ino
- set_adc() : LTC68041.cpp , LTC68041.h , LTC68042.cpp , LTC68042.h
- set_adc_scaling_factor() : DC2423A.ino
- set_CS_decoder() : LTC24XX_general_test.ino
- set_frequency() : DC726B_A.ino , DC726B_B.ino
- set_gain() : DC1410AB.ino , DC1410AA.ino
- set_LTC6945_ALLREGS() : LTC6945.cpp , LTC6945.h
- set_LTC6945_global_fref() : LTC6945.cpp , LTC6945.h
- set_LTC6945_global_frf() : LTC6945.cpp , LTC6945.h
- set_LTC6945_global_vcolim() : LTC6945.cpp , LTC6945.h
- set_LTC6945_SPI_FIELD() : LTC6945.cpp , LTC6945.h
- set_LTC6946_ALLREGS() : LTC6946.cpp , LTC6946.h
- set_LTC6946_global_fref() : LTC6946.cpp , LTC6946.h
- set_LTC6946_global_frf() : LTC6946.cpp , LTC6946.h
- set_LTC6946_SPI_FIELD() : LTC6946.cpp , LTC6946.h
- set_LTC6947_ALLREGS() : LTC6947.cpp , LTC6947.h
- set_LTC6947_global_fref() : LTC6947.cpp , LTC6947.h
- set_LTC6947_global_frf() : LTC6947.cpp , LTC6947.h
- set_LTC6947_global_vcolim() : LTC6947.cpp , LTC6947.h
- set_LTC6947_SPI_FIELD() : LTC6947.cpp , LTC6947.h
- set_LTC6948_ALLREGS() : LTC6948.cpp , LTC6948.h
- set_LTC6948_global_fref() : LTC6948.cpp , LTC6948.h
- set_LTC6948_global_frf() : LTC6948.cpp , LTC6948.h
- set_LTC6948_SPI_FIELD() : LTC6948.cpp , LTC6948.h
- set_LTC6950_ALLREGS() : LTC6950.cpp , LTC6950.h
- set_LTC6950_global_fref() : LTC6950.cpp , LTC6950.h
- set_LTC6950_global_frf() : LTC6950.cpp , LTC6950.h
- set_LTC6950_global_vcolim() : LTC6950.h , LTC6950.cpp
- set_LTC6950_SPI_FIELD() : LTC6950.cpp , LTC6950.h
- set_LTC6951_ALLREGS() : LTC6951.cpp , LTC6951.h
- set_LTC6951_REGS_freq_jump() : LTC6951.cpp , LTC6951.h
- set_LTC6951_REGS_lkup_tbl() : LTC6951.cpp , LTC6951.h
- set_LTC6951_SPI_FIELD() : LTC6951.cpp , LTC6951.h
- set_LTC6952_REGS_lkup_tbl() : LTC6952.cpp , LTC6952.h
- set_LTC6952_SPI_FIELD() : LTC6952.cpp , LTC6952.h
- set_LTC6953_REGS_lkup_tbl() : LTC6953.cpp , LTC6953.h
- set_LTC6953_SPI_FIELD() : LTC6953.cpp , LTC6953.h
- set_LTC6954_ALLREGS() : LTC6954.cpp , LTC6954.h
- set_LTC6954_SPI_FIELD() : LTC6954.cpp , LTC6954.h
- set_output_high_voltage() : DC2978A.ino
- set_output_low_voltage() : DC2978A.ino
- set_output_voltage() : DC2978A.ino
- set_slew() : DC2978A.ino
- set_spi_freq() : bms_hardware.h
- set_voltage() : Precision_Voltage_Source.ino
- set_voltage_hex() : Precision_Voltage_Source.ino
- SetCurrent() : EasySMU_Run.ino
- setpoint : LT1054_voltage_mode_buck.ino , LT1054_voltage_mode_buck_DC_ctrl.ino
- setPwmFrequency() : LT1054_voltage_mode_buck.ino , LT1054_voltage_mode_buck_DC_ctrl.ino
- setThresh() : DC2218A.ino
- settings() : DC726B_A.ino , DC726B_B.ino , Audio_Spectrum_Analyzer.ino
- SETTLE_CHANNEL : DC2196A.ino , DC2025A.ino
- SETTLE_TRIGGER : DC2692A.ino , DC2196A.ino , DC2025A.ino
- setup() : DC998A.ino , DC1704A.ino , DC2024A.ino , DC2217A.ino , DC1811B.ino , DC1989A.ino , DC2693A.ino , DC2460A.ino , DC2091A.ino , DC2839A.ino , DC1304A_A.ino , DC1304A_B.ino , DC1651A.ino , DC1652A.ino , DC1894.ino , DC1942.ino , DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino , DC726B_A.ino , DC726B_B.ino , DC1649A.ino , DC1705C.ino , DC1846A.ino , DC1959A.ino , DC1795A.ino , DC2248A.ino , DC2609A.ino , DC2610A.ino , LTC24XX_general_test.ino , DC1954A.ino , DC2978A.ino , DC2423A.ino , DC2741_production_test.ino , CN-0413.ino , EVAL-AD5933.ino , EVAL-AD5686R.ino , EVAL-AD5696R.ino , EVAL-AD7124-8.ino , EVAL-ADT7420.ino , Audio_Spectrum_Analyzer.ino , device_logger.ino , User Contributed/DC1962C/faultlog/faultlog.ino , hello_world.ino , program.ino , rail_logger.ino , retention.ino , svid.ino , ultra_fix.ino , DC2430A.ino , DoxygenExample.ino , FAE_April_2013.ino , sandbox.ino , Precision_Voltage_Source.ino , Synth.ino , vmClock.ino , DC590B.ino , DC590B_enhanced.ino , I2C_Address_Scan.ino , MyBlink.ino , Serial_EEPROM_Test.ino , Speed_Test.ino , LT1054_voltage_mode_buck.ino , LT1054_voltage_mode_buck_DC_ctrl.ino , _24xx_iso_spi_delay.ino , _24xx_iso_spi_poll.ino , CN0416_capitalizer.ino , CN0416_echo_node.ino , CN0416_SerialPassthrough.ino , EasySMU_Run.ino , LTC2442_Datalogger.ino , LTC2449_Datalogger.ino , LTC2492_Panel_Meter.ino , LTC2492_Thermocouple_Meter.ino , CapTouchPaint.ino , breakouttouchpaint.ino , graphicstest.ino , onoffbutton.ino , onoffbutton_breakout.ino , spitftbitmap.ino , touchpaint.ino , touchScreen.ino , DC572A.ino , DC682A.ino , DC806A.ino , DC1339A.ino , DC1444A.ino , DC1186A.ino , DC1337A.ino , DC786A.ino , DC1563A.ino , DC1908A.ino , DC2094A.ino , DC1208A.ino , DC1190A.ino , DC1796A.ino , DC1813A.ino , DC2263A.ino , DC2071AA.ino , DC1925A.ino , DC1783A.ino , DC1805A.ino , DC1571A.ino , DC2289AA.ino , DC746A.ino , DC1976A.ino , DC571A.ino , DC570A.ino , DC1410AB.ino , DC1785A.ino , DC742A.ino , DC1490.ino , DC1491A.ino , DC2507A_MULTI_SENSOR_BOARD_THERMOCOUPLE_PT100_CJ.ino , DC1716A.ino , DC798B.ino , DC941A.ino , DC939A.ino , DC1009AA.ino , DC1011AB.ino , DC1012A_B.ino , 2986/DC2213_DEDICATED_RTD_BOARD/DC2213_DEDICATED_RTD_BOARD.ino , DC1011AA.ino , DC1410AA.ino , DC1012AA.ino , 2986/DC2211_RTD/DC2211_RTD.ino , DC2222_interrupt_driven_read.ino , DC2222AB.ino , DC2222AC.ino , DATASHEET_FIGURE_50.ino , DC579A.ino , DC809A.ino , DC935A.ino , DC934A.ino , DC1466.ino , DC1534A.ino , DC1333A.ino , 2986/DATASHEET_FIGURE_27/DATASHEET_FIGURE_27.ino , DC1096B.ino , DC2197.ino , Margining.ino , 2986/DATASHEET_FIGURE_18/DATASHEET_FIGURE_18.ino , DC1678A.ino , DC1703A.ino , DC1397A.ino , 2986/DATASHEET_CUSTOM_THERMISTOR_TABLE/DATASHEET_CUSTOM_THERMISTOR_TABLE.ino , DC1529A.ino , DC2692A.ino , DC2376A.ino , DC2196A.ino , DC2025A.ino , LTC2668_backpage_app.ino , DC1684AB.ino , 2984/DC2211_RTD/DC2211_RTD.ino , DC1684AA.ino , DC2364A.ino , DC1880A.ino , DATASHEET_FIGURE_34.ino , DC2405A.ino , DC1633B.ino , DC1605B.ino , 2984/DATASHEET_FIGURE_24/DATASHEET_FIGURE_24.ino , DC2313A.ino , DC1496BB.ino , DC1812AA.ino , DC1812A-B.ino , DC1697A.ino , DC2156.ino , DC2334A.ino , 2984/DATASHEET_CUSTOM_STEINHART_HART/DATASHEET_CUSTOM_STEINHART_HART.ino , DC2574A_KIT.ino , DC2467.ino , DC980.ino , 2983/DC2212_THERMOCOUPLE_BOARD/DC2212_THERMOCOUPLE_BOARD.ino , DC2875A.ino , DC2675A.ino , DC1978.ino , 2983/DC2210_EXPERIMENTER_BOARD/DC2210_EXPERIMENTER_BOARD.ino , Part Number/2000/2900/2974/faultlog/faultlog.ino , DC2022A.ino , DC2382.ino , Part Number/2000/2900/2975/faultlog/faultlog.ino , DC2028A.ino , Part Number/2000/2900/2977/faultlog/faultlog.ino , Part Number/2000/2900/2978/faultlog/faultlog.ino , 2983/DATASHEET_FIGURE_21/DATASHEET_FIGURE_21.ino , DC2198A.ino , Part Number/2000/2900/2980/faultlog/faultlog.ino , 2983/DATASHEET_CUSTOM_RTD/DATASHEET_CUSTOM_RTD.ino , 2983/DATASHEET_CUSTOM_STEINHART_HART/DATASHEET_CUSTOM_STEINHART_HART.ino , 2983/DATASHEET_CUSTOM_THERMISTOR_TABLE/DATASHEET_CUSTOM_THERMISTOR_TABLE.ino , 2983/DATASHEET_CUSTOM_THERMOCOUPLE/DATASHEET_CUSTOM_THERMOCOUPLE.ino , 2983/DATASHEET_FIGURE_12/DATASHEET_FIGURE_12.ino , 2983/DATASHEET_FIGURE_15/DATASHEET_FIGURE_15.ino , 2983/DATASHEET_FIGURE_18/DATASHEET_FIGURE_18.ino , DATASHEET_FIGURE_19.ino , 2983/DATASHEET_FIGURE_24/DATASHEET_FIGURE_24.ino , 2983/DATASHEET_FIGURE_27/DATASHEET_FIGURE_27.ino , 2983/DATASHEET_FIGURE_30/DATASHEET_FIGURE_30.ino , DATASHEET_FIGURE_31.ino , DATASHEET_FIGURE_32.ino , DATASHEET_FIGURE_6.ino , 2983/DATASHEET_FIGURE_9/DATASHEET_FIGURE_9.ino , 2983/DC2211_RTD/DC2211_RTD.ino , 2983/DC2211_THERMOCOUPLE/DC2211_THERMOCOUPLE.ino , 2983/DC2211_UNIVERSAL_TEMPERATURE_MEASUREMENT_BOARD/DC2211_UNIVERSAL_TEMPERATURE_MEASUREMENT_BOARD.ino , 2983/DC2213_DEDICATED_RTD_BOARD/DC2213_DEDICATED_RTD_BOARD.ino , 2983/DC2214_DEDICATED_THERMISTOR_BOARD/DC2214_DEDICATED_THERMISTOR_BOARD.ino , 2984/DATASHEET_CUSTOM_RTD/DATASHEET_CUSTOM_RTD.ino , 2984/DATASHEET_CUSTOM_THERMISTOR_TABLE/DATASHEET_CUSTOM_THERMISTOR_TABLE.ino , 2984/DATASHEET_CUSTOM_THERMOCOUPLE/DATASHEET_CUSTOM_THERMOCOUPLE.ino , 2984/DATASHEET_FIGURE_12/DATASHEET_FIGURE_12.ino , 2984/DATASHEET_FIGURE_15/DATASHEET_FIGURE_15.ino , 2984/DATASHEET_FIGURE_18/DATASHEET_FIGURE_18.ino , 2984/DATASHEET_FIGURE_21/DATASHEET_FIGURE_21.ino , 2984/DATASHEET_FIGURE_22/DATASHEET_FIGURE_22.ino , 2984/DATASHEET_FIGURE_27/DATASHEET_FIGURE_27.ino , 2984/DATASHEET_FIGURE_30/DATASHEET_FIGURE_30.ino , 2984/DATASHEET_FIGURE_33/DATASHEET_FIGURE_33.ino , DATASHEET_FIGURE_35.ino , 2984/DATASHEET_FIGURE_9/DATASHEET_FIGURE_9.ino , 2984/DC2210_EXPERIMENTER_BOARD/DC2210_EXPERIMENTER_BOARD.ino , 2984/DC2211_THERMOCOUPLE/DC2211_THERMOCOUPLE.ino , 2984/DC2211_UNIVERSAL_TEMPERATURE_MEASUREMENT_BOARD/DC2211_UNIVERSAL_TEMPERATURE_MEASUREMENT_BOARD.ino , 2984/DC2212_THERMOCOUPLE_BOARD/DC2212_THERMOCOUPLE_BOARD.ino , 2984/DC2213_DEDICATED_RTD_BOARD/DC2213_DEDICATED_RTD_BOARD.ino , 2984/DC2214_DEDICATED_THERMISTOR_BOARD/DC2214_DEDICATED_THERMISTOR_BOARD.ino , 2986/DATASHEET_CUSTOM_RTD/DATASHEET_CUSTOM_RTD.ino , 2986/DATASHEET_CUSTOM_STEINHART_HART/DATASHEET_CUSTOM_STEINHART_HART.ino , 2986/DATASHEET_CUSTOM_THERMOCOUPLE/DATASHEET_CUSTOM_THERMOCOUPLE.ino , 2986/DATASHEET_FIGURE_12/DATASHEET_FIGURE_12.ino , 2986/DATASHEET_FIGURE_15/DATASHEET_FIGURE_15.ino , 2986/DATASHEET_FIGURE_21/DATASHEET_FIGURE_21.ino , 2986/DATASHEET_FIGURE_22/DATASHEET_FIGURE_22.ino , 2986/DATASHEET_FIGURE_24/DATASHEET_FIGURE_24.ino , 2986/DATASHEET_FIGURE_30/DATASHEET_FIGURE_30.ino , 2986/DATASHEET_FIGURE_33/DATASHEET_FIGURE_33.ino , DATASHEET_FIGURE_39.ino , DATASHEET_FIGURE_42.ino , DATASHEET_FIGURE_45.ino , DATASHEET_FIGURE_48.ino , DATASHEET_FIGURE_49.ino , DATASHEET_FIGURE_51.ino , DATASHEET_FIGURE_52.ino , 2986/DC2210_EXPERIMENTER_BOARD/DC2210_EXPERIMENTER_BOARD.ino , 2986/DC2211_THERMOCOUPLE/DC2211_THERMOCOUPLE.ino , 2986/DC2211_UNIVERSAL_TEMPERATURE_MEASUREMENT_BOARD/DC2211_UNIVERSAL_TEMPERATURE_MEASUREMENT_BOARD.ino , 2986/DC2212_THERMOCOUPLE_BOARD/DC2212_THERMOCOUPLE_BOARD.ino , 2986/DC2214_DEDICATED_THERMISTOR_BOARD/DC2214_DEDICATED_THERMISTOR_BOARD.ino , DC2507A_MULTI_SENSOR_BOARD.ino , DC2507A_MULTI_SENSOR_BOARD_10K_THERMISTOR.ino , DC2507A_MULTI_SENSOR_BOARD_2_WIRE_RTD.ino , DC2507A_MULTI_SENSOR_BOARD_3_WIRE_RTD.ino , DC2507A_MULTI_SENSOR_BOARD_4_WIRE_RTD.ino , DC2507A_MULTI_SENSOR_BOARD_THERMOCOUPLE_10K_THERMISTOR_CJ.ino , DC2023A.ino , Part Number/2000/2900/2987/faultlog/faultlog.ino , DC1338.ino , DC2561.ino , DC2343A.ino , DC1558_DC1808.ino , DC1590B.ino , Part Number/3000/3800/3880/faultlog/faultlog.ino , DC1936A.ino , Part Number/3000/3800/3882/faultlog/faultlog.ino , DC1778A.ino , Part Number/3000/3800/3883/faultlog/faultlog.ino , DC2155A.ino , fast_telemetry.ino , Part Number/3000/3800/3887/faultlog/faultlog.ino , DC2218A.ino , DC1674A.ino , DC874A.ino , DC985A.ino
- setup_ser_mode() : DC2334A.ino
- SetVoltage() : EasySMU_Run.ino
- shdn_settings : DC1304A_A.ino , DC1304A_B.ino
- SHDNb : DC2364A.ino
- shift_count : DC1466.ino , DC1703A.ino , DC579A.ino , DC809A.ino , DC935A.ino , DC1534A.ino , DC1333A.ino , DC1678A.ino , DC1397A.ino , DC1529A.ino
- shl64() : LTC6950.h , LTC6945.h , LTC6947.h , LTC6945.cpp , LTC6946.cpp , LTC6946.h , LTC6947.cpp , LTC6948.cpp , LTC6948.h , LTC6950.cpp
- shl64by() : LTC6947.h , LTC6946.h , LTC6945.h , LTC6948.h , LTC6948.cpp , LTC6945.cpp , LTC6946.cpp , LTC6947.cpp , LTC6950.cpp , LTC6950.h
- shr64() : LTC6946.h , LTC6948.h , LTC6950.h , LTC6947.h , LTC6945.h , LTC6947.cpp , LTC6945.cpp , LTC6946.cpp , LTC6948.cpp , LTC6950.cpp
- shr64by() : LTC6945.h , LTC6946.cpp , LTC6948.h , LTC6950.h , LTC6946.h , LTC6945.cpp , LTC6947.cpp , LTC6947.h , LTC6948.cpp , LTC6950.cpp
- sidebend() : DC2218A.ino
- sidebendAuto() : DC2218A.ino
- sign : Precision_Voltage_Source.ino
- sign_extend_17() : LTC2348.cpp
- SIGRD : program.ino
- SINGLE_ENDED_CONFIG_ARRAY : LTC2449_Datalogger.ino , LTC24XX_general_test.ino
- single_ended_differential : DC1186A.ino , DC1444A.ino , DC682A.ino , DC1337A.ino
- SLOW : LTC2492_original.h
- SMBALERT_MASK : LT_PMBus.h
- smbus : DC1633B.ino , DC1605B.ino , DC2313A.ino , DC2467.ino , DC2875A.ino , DC1978.ino , DC2022A.ino , Part Number/2000/2900/2977/faultlog/faultlog.ino , Part Number/2000/2900/2978/faultlog/faultlog.ino , DC2198A.ino , DC2023A.ino , DC1936A.ino , DC1778A.ino , DC2155A.ino , DC2028A.ino , DC1674A.ino , DC1811B.ino , DC1989A.ino , User Contributed/DC1962C/faultlog/faultlog.ino , svid.ino , sandbox.ino , DC2675A.ino , Part Number/3000/3800/3880/faultlog/faultlog.ino , Part Number/2000/2900/2980/faultlog/faultlog.ino , Part Number/3000/3800/3883/faultlog/faultlog.ino , Part Number/3000/3800/3882/faultlog/faultlog.ino , Part Number/3000/3800/3887/faultlog/faultlog.ino , DC2978A.ino , retention.ino , ultra_fix.ino , DC980.ino , hello_world.ino , fast_telemetry.ino , DC2263A.ino , DC1590B.ino , Part Number/2000/2900/2987/faultlog/faultlog.ino , Part Number/2000/2900/2975/faultlog/faultlog.ino , program.ino , Part Number/2000/2900/2974/faultlog/faultlog.ino , DC2382.ino
- smbus_read_register : LTC4155.h
- smbus_write_register : LTC4155.h
- smbusNoPec : svid.ino , rail_logger.ino , program.ino , device_logger.ino
- smbusNoPec__ : nvm_data_helpers.h , nvm.h , main_record_processor.h , nvm.cpp
- smbusPec : svid.ino , rail_logger.ino , program.ino , device_logger.ino
- smbusPec__ : nvm.cpp , nvm_data_helpers.h , main_record_processor.h , nvm.h
- smoothing_const : DC1410AA.ino , DC1410AB.ino
- SMU : EasySMU_Run.ino
- SNEAKER_PORT_ADDRESS : LTC2508.h , LTC2512.h
- SNEAKER_PORT_I2C_ADDRESS : LTC2348.h
- sneaker_port_init() : DC2222_interrupt_driven_read.ino , DC2094A.ino , DC2222AC.ino , DC2222AB.ino
- SOFTSPAN : LTC2348.h
- spi_begin : Adafruit_ILI9341.cpp
- SPI_CPHA : platform_drivers.h
- SPI_CPOL : platform_drivers.h
- spi_disable() : LT_SPI.h , LT_SPI.cpp
- spi_divider : DC590B.ino , DC590B_enhanced.ino , DC2430A.ino
- spi_enable() : LT_SPI.cpp , LT_SPI.h
- spi_end : Adafruit_ILI9341.cpp
- spi_init() : platform_drivers.h , platform_drivers.cpp
- spi_init_param : platform_drivers.h
- spi_mode : DC590B.ino , DC2430A.ino , DC590_subset.ino , DC590B_enhanced.ino
- spi_out : DC1304A_B.ino , DC1304A_A.ino
- spi_params : EVAL-AD5696R.ino , EVAL-AD5686R.ino , EVAL-AD7124-8.ino
- spi_read() : LT_SPI.cpp , LT_SPI.h
- spi_read_byte() : bms_hardware.cpp , bms_hardware.h
- spi_remove() : platform_drivers.cpp , platform_drivers.h
- spi_transfer_block() : LT_SPI.h , LT_SPI.cpp
- spi_transfer_byte() : LT_SPI.cpp , LT_SPI.h
- spi_transfer_word() : LT_SPI.cpp , LT_SPI.h
- spi_type : platform_drivers.h
- spi_write() : LT_SPI.h , LT_SPI.cpp
- spi_write_and_read() : platform_drivers.cpp , platform_drivers.h
- spi_write_array() : LTC68031.cpp , bms_hardware.cpp , bms_hardware.h , LTC68032.cpp , LTC68041.cpp , LTC68031.h , LTC68042.cpp , LTC68041.h , LTC68032.h , LTC68042.h
- spi_write_read() : LTC68032.h , LTC68032.cpp , LTC68041.cpp , LTC68031.h , bms_hardware.cpp , LTC68031.cpp , LTC68041.h , bms_hardware.h , LTC68042.cpp , LTC68042.h
- SPLASH_SCREEN_DELAY : DC2574A_KIT.ino
- start : Audio_Spectrum_Analyzer.ino
- start_millis : DC2839A.ino
- startMinutes : vmClock.ino
- startsequence : DC2218A.ino
- startup : DC2218A.ino
- STAT : LTC6811.h , LTC681x.h , LTC6812.h , LTC6813.h , LTC6810.h
- STAT_CH_ALL : LTC681x.h
- STAT_CH_ITEMP : LTC681x.h
- STAT_CH_SOC : LTC681x.h
- STAT_CH_TO_CONVERT : DC2259.ino , DC2515.ino , DC2350AB.ino , DC2350AA.ino
- STAT_CH_VREGA : LTC681x.h
- STAT_CH_VREGD : LTC681x.h
- state : LT1054_voltage_mode_buck_DC_ctrl.ino
- status() : DC2364A.ino
- STATUS_ADDRESS_READ_ACK : LT_I2C_Wire.h , LT_I2C.h
- STATUS_ADDRESS_READ_NACK : LT_I2C_Wire.h , LT_I2C.h
- STATUS_ADDRESS_WRITE_ACK : LT_I2C_Wire.h , LT_I2C.h
- STATUS_ADDRESS_WRITE_NACK : LT_I2C_Wire.h , LT_I2C.h
- STATUS_ARBITRATION_LOST : LT_I2C.h , LT_I2C_Wire.h
- STATUS_BYTE : LT_PMBus.h , retention.ino
- STATUS_CML : LT_PMBus.h , retention.ino
- STATUS_CML_CMD_FAULT : retention.ino , LT_PMBus.h
- STATUS_CML_DATA_FAULT : LT_PMBus.h , retention.ino
- STATUS_CML_MEM_FAULT : retention.ino , LT_PMBus.h
- STATUS_CML_PEC_FAULT : retention.ino , LT_PMBus.h
- STATUS_CML_PMBUS_FAULT : retention.ino , LT_PMBus.h
- STATUS_CML_PROC_FAULT : retention.ino , LT_PMBus.h
- STATUS_CML_UNKNOWN_FAULT : LT_PMBus.h , retention.ino
- STATUS_INPUT : LT_PMBus.h
- STATUS_IOUT : LT_PMBus.h
- STATUS_MFR_SPECIFIC : retention.ino , LT_PMBus.h
- STATUS_MFR_SPECIFIC_NVM_CRC : retention.ino
- STATUS_READ_ACK : LT_I2C_Wire.h , LT_I2C.h
- STATUS_READ_NACK : LT_I2C.h , LT_I2C_Wire.h
- STATUS_REPEATED_START : LT_I2C_Wire.h , LT_I2C.h
- STATUS_START : LT_I2C_Wire.h , LT_I2C.h
- STATUS_TEMP : LT_PMBus.h
- STATUS_VOUT : LT_PMBus.h
- STATUS_WORD : LT_PMBus.h , retention.ino
- STATUS_WORD_POWER_GOOD_B : retention.ino
- STATUS_WRITE_ACK : LT_I2C_Wire.h , LT_I2C.h
- STATUS_WRITE_NACK : LT_I2C.h , LT_I2C_Wire.h
- statusRegs : DC2574A_KIT.ino
- statusRegsRead : DC2574A_KIT.ino
- steeringRightAndLeft() : DC2218A.ino
- step : Audio_Spectrum_Analyzer.ino
- stimulus : DC2741_production_test.ino
- STMPE_CS : onoffbutton.ino , touchpaint.ino
- stop : Audio_Spectrum_Analyzer.ino
- store() : retention.ino
- store_alert_settings() : DC1496BB.ino , DC1697A.ino , DC2156.ino , DC1812AA.ino , DC1812A-B.ino
- store_calibration() : DC571A.ino , DC1397A.ino , DC1703A.ino , DC742A.ino , DC939A.ino , DC1678A.ino , DC1333A.ino , DC806A.ino , Audio_Spectrum_Analyzer.ino , DC1491A.ino , DC1529A.ino
- store_fault_logs() : retention.ino
- store_settings() : Synth.ino
- STORE_USER_ALL : retention.ino , LT_PMBus.h
- STORED_REF_STATE_BASE : DC1397A.ino , DC1703A.ino , DC1529A.ino , DC1678A.ino , DC1333A.ino , DC1534A.ino
- sub64() : LTC6947.cpp , LTC6948.h , LTC6948.cpp , LTC6946.h , LTC6950.cpp , LTC6945.h , LTC6945.cpp , LTC6946.cpp , LTC6950.h , LTC6947.h
- SUCCEED : DC2313A.ino
- SUCCESS : platform_drivers.h , LT_SMBus.h , LT_PMBus.h , record_type_basic_definitions.h
- SW_I2C_FREQUENCY : I2C_Address_Scan.ino , DC2741_production_test.ino
- SYSTEM_AFTER_VERIFY : record_type_definitions.h
- SYSTEM_BEFORE_PROGRAM : record_type_definitions.h
- SYSTEM_BEFORE_VERIFY : record_type_definitions.h