| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - r -

- railCnt_ : LT_PMBusDetect
- railDef_ : LT_PMBusRail
- rails_ : LT_PMBusDetect
- read() : LT_2974FaultLog , LT_2975FaultLog , LT_2977FaultLog , LT_2978FaultLog , LT_3880FaultLog , LT_3882FaultLog , LT_3883FaultLog , LT_3887FaultLog , LT_FaultLog
- read_iin : LT_2975FaultLog::IinData , LT_3880FaultLog::FaultLogReadLoopLtc3880 , LT_3883FaultLog::FaultLogReadLoopLtc3883 , LT_3887FaultLog::FaultLogReadLoopLtc3887
- read_iin_chan_p1 : LT_3883FaultLog::FaultLogReadLoopLtc3883
- read_iout : LT_2974FaultLog::IoutData , LT_2975FaultLog::IoutData
- read_iout_p0 : LT_3880FaultLog::FaultLogReadLoopLtc3880 , LT_3882FaultLog::FaultLogReadLoopLtc3882 , LT_3883FaultLog::FaultLogReadLoopLtc3883 , LT_3887FaultLog::FaultLogReadLoopLtc3887
- read_iout_p1 : LT_3880FaultLog::FaultLogReadLoopLtc3880 , LT_3882FaultLog::FaultLogReadLoopLtc3882 , LT_3887FaultLog::FaultLogReadLoopLtc3887
- read_pin : LT_2975FaultLog::PinData
- read_pout : LT_2974FaultLog::PoutData , LT_2975FaultLog::PoutData
- read_register : LTC4155_chip_cfg_t
- read_temp1 : LT_2974FaultLog::TempData , LT_2975FaultLog::TempData , LT_2978FaultLog::TempData
- read_temp2 : LT_2974FaultLog::FaultLogReadLoopLtc2974 , LT_2975FaultLog::FaultLogReadLoopLtc2975
- read_temperature_1_p0 : LT_3880FaultLog::FaultLogTelemetrySummaryLtc3880 , LT_3882FaultLog::FaultLogTelemetrySummaryLtc3882 , LT_3883FaultLog::FaultLogTelemetrySummaryLtc3883 , LT_3887FaultLog::FaultLogTelemetrySummaryLtc3887
- read_temperature_1_p1 : LT_3880FaultLog::FaultLogTelemetrySummaryLtc3880 , LT_3882FaultLog::FaultLogTelemetrySummaryLtc3882 , LT_3887FaultLog::FaultLogTelemetrySummaryLtc3887
- read_temperature_1_peak_p0 : LT_3883FaultLog::FaultLogTelemetrySummaryLtc3883
- read_temperature_2 : LT_3880FaultLog::FaultLogTelemetrySummaryLtc3880 , LT_3882FaultLog::FaultLogTelemetrySummaryLtc3882 , LT_3883FaultLog::FaultLogTelemetrySummaryLtc3883 , LT_3887FaultLog::FaultLogTelemetrySummaryLtc3887
- read_vin : LT_3880FaultLog::FaultLogReadLoopLtc3880 , LT_3882FaultLog::FaultLogReadLoopLtc3882 , LT_3883FaultLog::FaultLogReadLoopLtc3883 , LT_3887FaultLog::FaultLogReadLoopLtc3887
- read_vout : LT_2974FaultLog::VoutData , LT_2975FaultLog::VoutData , LT_2977FaultLog::VoutData , LT_2978FaultLog::VoutData
- read_vout_p0 : LT_3880FaultLog::FaultLogReadLoopLtc3880 , LT_3882FaultLog::FaultLogReadLoopLtc3882 , LT_3883FaultLog::FaultLogReadLoopLtc3883 , LT_3887FaultLog::FaultLogReadLoopLtc3887
- read_vout_p1 : LT_3880FaultLog::FaultLogReadLoopLtc3880 , LT_3882FaultLog::FaultLogReadLoopLtc3882 , LT_3887FaultLog::FaultLogReadLoopLtc3887
- readAlert() : LT_SMBus , LT_SMBusBase
- readBlock() : LT_SMBus , LT_SMBusBase , LT_SMBusGroup
- readBlockData() : LT_I2CBus
- readBlockDataPec() : LT_I2CBus
- readByte() : LT_I2CBus , LT_SMBus , LT_SMBusBase , LT_SMBusGroup
- readByteData() : LT_I2CBus
- ReadCalibration() : EasySMU
- readCmlStatusByte() : LT_PMBus
- readcommand8() : Adafruit_ILI9341
- readData() : Adafruit_FT6206
- readdata() : Adafruit_ILI9341
- readDutyCycle() : LT_PMBus , LT_PMBusDevice , LT_PMBusRail
- readEfficiency() : LT_PMBusRail
- readExternalTemperature() : LT_PMBus , LT_PMBusDevice , LT_PMBusRail
- readIin() : LT_PMBus , LT_PMBusDevice , LT_PMBusRail
- readInputStatusByte() : LT_PMBus
- readInternalTemperature() : LT_PMBus , LT_PMBusDevice , LT_PMBusRail
- readIout() : LT_PMBus , LT_PMBusDevice , LT_PMBusRail
- readIoutStatusByte() : LT_PMBus
- readIoutWithPage() : LT_PMBus
- readIoutWithPagePlus() : LT_PMBus
- readItemp() : LT_PMBus
- readMfrFaultLogStatusByte() : LT_FaultLog , LT_PMBus
- readMfrPads() : LT_PMBus
- readMfrSpecialId() : LT_PMBus , LT_PMBusDevice , LT_PMBusRail
- readMfrStatusByte() : LT_FaultLog , LT_PMBus
- readModel() : LT_PMBus
- readOtemp() : LT_PMBus
- readOtempWithPage() : LT_PMBus
- readOtempWithPagePlus() : LT_PMBus
- readPhaseBalance() : LT_PMBusRail
- readPin() : LT_PMBus , LT_PMBusDevice , LT_PMBusRail
- readPmbusRevision() : LT_PMBus
- readPout() : LT_PMBus , LT_PMBusDevice , LT_PMBusRail
- readPoutWithPage() : LT_PMBus
- readPoutWithPagePlus() : LT_PMBus
- readRegister8() : Adafruit_FT6206
- readRevision() : LT_PMBus
- readStatusByte() : LT_PMBus
- readStatusByteWithPage() : LT_PMBus
- readStatusByteWithPagePlus() : LT_PMBus
- readStatusCml() : LT_PMBus
- readStatusWord() : LT_PMBus , LT_PMBusDevice , LT_PMBusRail
- readStatusWordWithPage() : LT_PMBus
- readStatusWordWithPagePlus() : LT_PMBus
- readTemperatureStatusByte() : LT_PMBus
- readTransient() : LT_PMBusRail
- readVin() : LT_PMBus , LT_PMBusDevice , LT_PMBusRail
- readVout() : LT_PMBus , LT_PMBusDevice , LT_PMBusRail
- readVoutStatusByte() : LT_PMBus
- readVoutWithPage() : LT_PMBus
- readVoutWithPagePlus() : LT_PMBus
- readWord() : LT_SMBus , LT_SMBusBase , LT_SMBusGroup
- readWordData() : LT_I2CBus
- record : _InCircuitProgrammingRecordTypeListItem
- RecordType : tRecordHeader
- reference_mode : eeprom_data_union::data_struct_type
- release() : LT_2974FaultLog , LT_2975FaultLog , LT_2977FaultLog , LT_2978FaultLog , LT_3880FaultLog , LT_3882FaultLog , LT_3883FaultLog , LT_3887FaultLog , LT_FaultLog
- requestFrom() : LT_TwoWire
- reserved : LT_2974FaultLog::FaultLogReadLoopLtc2974 , LT_2975FaultLog::FaultLogReadLoopLtc2975 , LT_2978FaultLog::FaultLogReadLoopLtc2978
- reserved2 : LT_2978FaultLog::FaultLogReadLoopLtc2978
- reset() : LT_PMBus
- ResetCalibration() : EasySMU
- resetGlobal() : LT_PMBus
- RestoreFactoryCalibration() : EasySMU
- restoreFromNvm() : LT_PMBus
- restoreFromNvmAll() : LT_PMBus
- restoreFromNvmGlobal() : LT_PMBus
- rotation : Adafruit_GFX
- running_pec_ : LT_SMBus
- rx_data : ic_register
- rx_pec_match : ic_register