| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Public Member Functions | Data Fields
LT_2978FaultLog::FaultLogLtc2978 Struct Reference

## Detailed Description

Definition at line 154 of file LT_2978FaultLog.h.

## Public Member Functions
bool | isValidData (void *pos, uint8_t size=2)

## Data Fields
struct FaultLogPreambleLtc2978 | preamble
uint8_t | telemetryData [208]
struct FaultLogReadLoopLtc2978 * | loops
uint8_t | firstValidByte
uint8_t | lastValidByte

## Member Function Documentation

## ◆ isValidData()

bool LT_2978FaultLog::FaultLogLtc2978::isValidData | ( | void * | pos,
|  | uint8_t | size = `2`
| ) |  |

Definition at line 70 of file LT_2978FaultLog.cpp.

## Field Documentation

## ◆ firstValidByte

uint8_t LT_2978FaultLog::FaultLogLtc2978::firstValidByte

Definition at line 160 of file LT_2978FaultLog.h.

## ◆ lastValidByte

uint8_t LT_2978FaultLog::FaultLogLtc2978::lastValidByte

Definition at line 161 of file LT_2978FaultLog.h.

## ◆ loops

struct FaultLogReadLoopLtc2978* LT_2978FaultLog::FaultLogLtc2978::loops

Definition at line 159 of file LT_2978FaultLog.h.

## ◆ preamble

struct FaultLogPreambleLtc2978 LT_2978FaultLog::FaultLogLtc2978::preamble

Definition at line 157 of file LT_2978FaultLog.h.

## ◆ telemetryData

uint8_t LT_2978FaultLog::FaultLogLtc2978::telemetryData[208]

Definition at line 158 of file LT_2978FaultLog.h.

The documentation for this struct was generated from the following files:

- LT_2978FaultLog.h
- LT_2978FaultLog.cpp