| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
USBSNS_GOOD
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

USBSNS_GOOD Bit Field. More...

## Macros
#define | LTC4155_USBSNS_GOOD_SUBADDR LTC4155_REG4_SUBADDR
| USBSNS_GOOD More...
#define | LTC4155_USBSNS_GOOD_SIZE 1
#define | LTC4155_USBSNS_GOOD_OFFSET 6
#define | LTC4155_USBSNS_GOOD_MASK 0x40
#define | LTC4155_USBSNS_GOOD (LTC4155_USBSNS_GOOD_OFFSET << 12 | (LTC4155_USBSNS_GOOD_SIZE - 1) << 8 | LTC4155_USBSNS_GOOD_SUBADDR)

## Detailed Description

USBSNS_GOOD Bit Field.

USB input voltage valid.

- Register: REG4
- CommandCode: 0x04
- Size: 1
- Offset: 6
- MSB: 6
- MASK: 0x40
- Access: R
- Default: n/a

## Macro Definition Documentation

## ◆ LTC4155_USBSNS_GOOD

#define LTC4155_USBSNS_GOOD (LTC4155_USBSNS_GOOD_OFFSET << 12 | (LTC4155_USBSNS_GOOD_SIZE - 1) << 8 | LTC4155_USBSNS_GOOD_SUBADDR)

Definition at line 616 of file LTC4155_reg_defs.h.

## ◆ LTC4155_USBSNS_GOOD_MASK

#define LTC4155_USBSNS_GOOD_MASK 0x40

Definition at line 615 of file LTC4155_reg_defs.h.

## ◆ LTC4155_USBSNS_GOOD_OFFSET

#define LTC4155_USBSNS_GOOD_OFFSET 6

Definition at line 614 of file LTC4155_reg_defs.h.

## ◆ LTC4155_USBSNS_GOOD_SIZE

#define LTC4155_USBSNS_GOOD_SIZE 1

Definition at line 613 of file LTC4155_reg_defs.h.

## ◆ LTC4155_USBSNS_GOOD_SUBADDR

#define LTC4155_USBSNS_GOOD_SUBADDR LTC4155_REG4_SUBADDR

USBSNS_GOOD

Definition at line 612 of file LTC4155_reg_defs.h.