| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
REG2
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

REG2 Register. More...

## Macros
#define | LTC4155_REG2_SUBADDR 0x02
#define | LTC4155_REG2 (0 << 12 | (16 - 1) << 8 | LTC4155_REG2_SUBADDR)

## Detailed Description

REG2 Register.

7:4 | 3:2 | 1:0
--- | --- | ---
ICHARGE | VFLOAT | CXSET

- CommandCode: 0x02
- Contains Bit Fields:
  - ICHARGE : Battery charger current limit setting.
  - VFLOAT : Battery charge voltage setting.
  - CXSET : End-of-Charge indication current threshold setting. This threshold can also be used for charge termination if TIMER is set to 8_Hour_or_CoverX.

## Macro Definition Documentation

## ◆ LTC4155_REG2

#define LTC4155_REG2 (0 << 12 | (16 - 1) << 8 | LTC4155_REG2_SUBADDR)

Definition at line 323 of file LTC4155_reg_defs.h.

## ◆ LTC4155_REG2_SUBADDR

#define LTC4155_REG2_SUBADDR 0x02

Definition at line 322 of file LTC4155_reg_defs.h.