| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

### - r -

- read16() : spitftbitmap.ino
- read32() : spitftbitmap.ino
- read_68() : LTC681x.h , LTC681x.cpp
- read_bytes() : DC2218A.ino , retention.ino
- read_calibration() : LTC2492_Thermocouple_Meter.ino , LTC2492_original.h
- read_char() : UserInterface.cpp , UserInterface.h
- read_data() : UserInterface.cpp , UserInterface.h
- read_data_ISR() : DC2222_interrupt_driven_read.ino
- read_float() : UserInterface.cpp , UserInterface.h
- read_hex() : DC590_subset.ino , DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino , DC2430A.ino , DC590B.ino , DC590B_enhanced.ino
- read_input_current() : DC2978A.ino
- read_input_voltage() : DC2978A.ino
- read_int() : UserInterface.cpp , UserInterface.h
- read_LTC2442() : LTC2442_Datalogger.ino
- read_LTC2449() : LTC2449_Datalogger.ino
- read_LTC2492() : LTC2492_original.h , LTC2492_Thermocouple_Meter.ino
- read_output_current() : DC2978A.ino
- read_output_voltage() : DC2978A.ino
- read_quikeval_id_string() : QuikEval_EEPROM.cpp , QuikEval_EEPROM.h , QuikEval_EEPROM_Wire.cpp , QuikEval_EEPROM_Wire.h
- read_reg_map() : DC1976A.ino
- read_register() : DC1674A.ino
- read_status() : DC2978A.ino
- read_string() : UserInterface.cpp , UserInterface.h
- read_switches() : Precision_Voltage_Source.ino , Synth.ino
- read_voltage_or_resistance_results() : support_functions_LTC2983.cpp , support_functions_LTC2983.h , support_functions_LTC2984.cpp , support_functions_LTC2984.h , support_functions_LTC2986.cpp , support_functions_LTC2986.h
- readItemp() : retention.ino
- readItemp2977_8() : retention.ino
- ReadLine() : EasySMU_Run.ino
- readpot() : DC2218A.ino
- readThenVerifyNvmData() : nvm_data_helpers.cpp , nvm_data_helpers.h
- recordProcessor___0x01___processWriteByteOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x02___processWriteWordOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x04___processReadByteExpectOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x05___processReadWordExpectOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x09___bufferNVMData() : main_record_processor.cpp
- recordProcessor___0x0A___processReadByteLoopMaskOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x0B___processReadWordLoopMaskOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x0C___processPollReadByteUntilAckNoPEC() : main_record_processor.cpp
- recordProcessor___0x0D___processDelayMs() : main_record_processor.cpp
- recordProcessor___0x0E___processSendByteOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x0F___processWriteByteNoPEC() : main_record_processor.cpp
- recordProcessor___0x10___processWriteWordNoPEC() : main_record_processor.cpp
- recordProcessor___0x12___processReadByteExpectNoPEC() : main_record_processor.cpp
- recordProcessor___0x13___processReadWordExpectNoPEC() : main_record_processor.cpp
- recordProcessor___0x15___processReadByteLoopMaskNoPEC() : main_record_processor.cpp
- recordProcessor___0x16___processReadWordLoopMaskNoPEC() : main_record_processor.cpp
- recordProcessor___0x17___processSendByteNoPEC() : main_record_processor.cpp
- recordProcessor___0x18___processEvent() : main_record_processor.cpp
- recordProcessor___0x19___processReadByteExpectMaskNoPEC() : main_record_processor.cpp
- recordProcessor___0x1A___processReadWordExpectMaskNoPEC() : main_record_processor.cpp
- recordProcessor___0x1B___processVariableMetaData() : main_record_processor.cpp
- recordProcessor___0x1C___modifyWordNoPEC() : main_record_processor.cpp
- recordProcessor___0x1D___modifyByteNoPEC() : main_record_processor.cpp
- recordProcessor___0x1E___writeNvmData() : main_record_processor.cpp
- recordProcessor___0x1F___read_then_verifyNvmData() : main_record_processor.cpp
- recordProcessor___0x20___modifyByteOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x21___modifyWordOptionalPEC() : main_record_processor.cpp
- redBtn() : onoffbutton.ino , onoffbutton_breakout.ino
- reg_test() : DC1880A.ino
- reset() : DC2978A.ino
- reset_all_devices() : program.ino
- reset_parse_hex() : hex_file_parser.cpp , hex_file_parser.h
- restore() : retention.ino
- restore_alert_settings() : DC1812A-B.ino , DC1812AA.ino , DC1496BB.ino , DC2156.ino , DC1697A.ino
- restore_calibration() : DC1491A.ino , DC1466.ino , DC1678A.ino , DC1534A.ino , DC1703A.ino , DC571A.ino , DC1529A.ino , DC939A.ino , DC1397A.ino , DC1333A.ino , Audio_Spectrum_Analyzer.ino , DC806A.ino , DC742A.ino
- restore_dac_from_eeprom() : DC2692A.ino , DC2025A.ino , DC2376A.ino , DC2196A.ino
- restore_nvm() : program.ino
- restore_settings() : Synth.ino
- reverse_isospi_direction() : DC2515.ino
- rotate() : LT_2974FaultLog.cpp
- run_command() : DC2350AA.ino , DC1651A.ino , DC1652A.ino , DC2515.ino , DC1942.ino , DC1894.ino , DC2259.ino , DC2350AB.ino