| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
OTG_ENABLED
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

OTG_ENABLED Bit Field. More...

## Macros
#define | LTC4155_OTG_ENABLED_SUBADDR LTC4155_REG3_SUBADDR
| OTG_ENABLED More...
#define | LTC4155_OTG_ENABLED_SIZE 1
#define | LTC4155_OTG_ENABLED_OFFSET 3
#define | LTC4155_OTG_ENABLED_MASK 0x08
#define | LTC4155_OTG_ENABLED (LTC4155_OTG_ENABLED_OFFSET << 12 | (LTC4155_OTG_ENABLED_SIZE - 1) << 8 | LTC4155_OTG_ENABLED_SUBADDR)

## Detailed Description

OTG_ENABLED Bit Field.

On-the-Go boost converter enable status.

- Register: REG3
- CommandCode: 0x03
- Size: 1
- Offset: 3
- MSB: 3
- MASK: 0x08
- Access: R
- Default: n/a

## Macro Definition Documentation

## ◆ LTC4155_OTG_ENABLED

#define LTC4155_OTG_ENABLED (LTC4155_OTG_ENABLED_OFFSET << 12 | (LTC4155_OTG_ENABLED_SIZE - 1) << 8 | LTC4155_OTG_ENABLED_SUBADDR)

Definition at line 503 of file LTC4155_reg_defs.h.

## ◆ LTC4155_OTG_ENABLED_MASK

#define LTC4155_OTG_ENABLED_MASK 0x08

Definition at line 502 of file LTC4155_reg_defs.h.

## ◆ LTC4155_OTG_ENABLED_OFFSET

#define LTC4155_OTG_ENABLED_OFFSET 3

Definition at line 501 of file LTC4155_reg_defs.h.

## ◆ LTC4155_OTG_ENABLED_SIZE

#define LTC4155_OTG_ENABLED_SIZE 1

Definition at line 500 of file LTC4155_reg_defs.h.

## ◆ LTC4155_OTG_ENABLED_SUBADDR

#define LTC4155_OTG_ENABLED_SUBADDR LTC4155_REG3_SUBADDR

OTG_ENABLED

Definition at line 499 of file LTC4155_reg_defs.h.