| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
ENABLE_OTG_INT
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

ENABLE_OTG_INT Bit Field. More...

## Macros
#define | LTC4155_ENABLE_OTG_INT_SUBADDR LTC4155_REG6_SUBADDR
| ENABLE_OTG_INT More...
#define | LTC4155_ENABLE_OTG_INT_SIZE 1
#define | LTC4155_ENABLE_OTG_INT_OFFSET 4
#define | LTC4155_ENABLE_OTG_INT_MASK 0x10
#define | LTC4155_ENABLE_OTG_INT (LTC4155_ENABLE_OTG_INT_OFFSET << 12 | (LTC4155_ENABLE_OTG_INT_SIZE - 1) << 8 | LTC4155_ENABLE_OTG_INT_SUBADDR)

## Detailed Description

ENABLE_OTG_INT Bit Field.

Enable ID_PIN_DETECT and OTG_ENABLED USB On-The-Go interrupts.

- Register: REG6
- CommandCode: 0x06
- Size: 1
- Offset: 4
- MSB: 4
- MASK: 0x10
- Access: R/W
- Default: 0

## Macro Definition Documentation

## ◆ LTC4155_ENABLE_OTG_INT

#define LTC4155_ENABLE_OTG_INT (LTC4155_ENABLE_OTG_INT_OFFSET << 12 | (LTC4155_ENABLE_OTG_INT_SIZE - 1) << 8 | LTC4155_ENABLE_OTG_INT_SUBADDR)

Definition at line 913 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_OTG_INT_MASK

#define LTC4155_ENABLE_OTG_INT_MASK 0x10

Definition at line 912 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_OTG_INT_OFFSET

#define LTC4155_ENABLE_OTG_INT_OFFSET 4

Definition at line 911 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_OTG_INT_SIZE

#define LTC4155_ENABLE_OTG_INT_SIZE 1

Definition at line 910 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_OTG_INT_SUBADDR

#define LTC4155_ENABLE_OTG_INT_SUBADDR LTC4155_REG6_SUBADDR

ENABLE_OTG_INT

Definition at line 909 of file LTC4155_reg_defs.h.