| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

### - t -

- temp_to_code() : EVAL-ADT7420.ino
- test() : DC2197.ino , Audio_Spectrum_Analyzer.ino
- test_all() : LTC24XX_general_test.ino
- test_LTC2400() : LTC24XX_general_test.ino
- test_LTC2412() : LTC24XX_general_test.ino
- test_LTC2418() : LTC24XX_general_test.ino
- test_LTC2420() : LTC24XX_general_test.ino
- test_LTC2436() : LTC24XX_general_test.ino
- test_LTC2439() : LTC24XX_general_test.ino
- test_LTC2449() : LTC24XX_general_test.ino
- test_LTC2494() : LTC24XX_general_test.ino
- test_LTC2495() : LTC24XX_general_test.ino
- test_LTC2496() : LTC24XX_general_test.ino
- test_LTC2497() : LTC24XX_general_test.ino
- test_LTC2498() : LTC24XX_general_test.ino
- test_LTC2499() : LTC24XX_general_test.ino
- testCircles() : graphicstest.ino
- testFastLines() : graphicstest.ino
- testFilledCircles() : graphicstest.ino
- testFilledRects() : graphicstest.ino
- testFilledRoundRects() : graphicstest.ino
- testFilledTriangles() : graphicstest.ino
- testFillScreen() : graphicstest.ino
- testLines() : graphicstest.ino
- testRects() : graphicstest.ino
- testRoundRects() : graphicstest.ino
- testText() : graphicstest.ino
- testTriangles() : graphicstest.ino
- tinyDC590B() : DC590_subset.ino
- toggle_pg0() : DC2675A.ino , DC2875A.ino
- toggle_pg1() : DC2875A.ino , DC2675A.ino
- toggle_pg2() : DC2675A.ino , DC2875A.ino
- toggle_pg3() : DC2875A.ino , DC2675A.ino
- transfer_byte() : support_functions_LTC2983.h , support_functions_LTC2984.h , support_functions_LTC2983.cpp , support_functions_LTC2986.h , support_functions_LTC2984.cpp , support_functions_LTC2986.cpp
- transfer_four_bytes() : support_functions_LTC2984.cpp , support_functions_LTC2983.cpp , support_functions_LTC2986.h , support_functions_LTC2986.cpp , support_functions_LTC2983.h , support_functions_LTC2984.h
- turn_off() : DC2978A.ino
- turn_on() : DC2978A.ino
- type_K_V2C() : LTC2492_Thermocouple_Meter.ino , LTC2492_original.h