| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Public Member Functions | Data Fields
LT_2974FaultLog::FaultLogLtc2974 Struct Reference

## Detailed Description

Definition at line 203 of file LT_2974FaultLog.h.

## Public Member Functions
bool | isValidData (void *pos, uint8_t size=2)

## Data Fields
struct FaultLogPreambleLtc2974 | preamble
uint8_t | telemetryData [184]
struct FaultLogReadLoopLtc2974 * | loops
uint8_t | firstValidByte
uint8_t | lastValidByte

## Member Function Documentation

## ◆ isValidData()

bool LT_2974FaultLog::FaultLogLtc2974::isValidData | ( | void * | pos,
|  | uint8_t | size = `2`
| ) |  |

Definition at line 107 of file LT_2974FaultLog.cpp.

## Field Documentation

## ◆ firstValidByte

uint8_t LT_2974FaultLog::FaultLogLtc2974::firstValidByte

Definition at line 209 of file LT_2974FaultLog.h.

## ◆ lastValidByte

uint8_t LT_2974FaultLog::FaultLogLtc2974::lastValidByte

Definition at line 210 of file LT_2974FaultLog.h.

## ◆ loops

struct FaultLogReadLoopLtc2974* LT_2974FaultLog::FaultLogLtc2974::loops

Definition at line 208 of file LT_2974FaultLog.h.

## ◆ preamble

struct FaultLogPreambleLtc2974 LT_2974FaultLog::FaultLogLtc2974::preamble

Definition at line 206 of file LT_2974FaultLog.h.

## ◆ telemetryData

uint8_t LT_2974FaultLog::FaultLogLtc2974::telemetryData[184]

Definition at line 207 of file LT_2974FaultLog.h.

The documentation for this struct was generated from the following files:

- LT_2974FaultLog.h
- LT_2974FaultLog.cpp