| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Data Fields
st Struct Reference

Status Reg data structure. More...

## Detailed Description

Status Reg data structure.

Definition at line 131 of file LTC681x.h.

## Data Fields
uint16_t | stat_codes [4]
| Status codes. More...
uint8_t | flags [3]
| Byte array that contains the uv/ov flag data. More...
uint8_t | mux_fail [1]
| Mux self test status flag. More...
uint8_t | thsd [1]
| Thermal shutdown status. More...
uint8_t | pec_match [2]
| If a PEC error was detected during most recent read cmd. More...

## Field Documentation

## ◆ flags

uint8_t st::flags[3]

Byte array that contains the uv/ov flag data.

Definition at line 134 of file LTC681x.h.

## ◆ mux_fail

uint8_t st::mux_fail[1]

Mux self test status flag.

Definition at line 135 of file LTC681x.h.

## ◆ pec_match

uint8_t st::pec_match[2]

If a PEC error was detected during most recent read cmd.

Definition at line 137 of file LTC681x.h.

## ◆ stat_codes

uint16_t st::stat_codes[4]

Status codes.

Definition at line 133 of file LTC681x.h.

## ◆ thsd

uint8_t st::thsd[1]

Thermal shutdown status.

Definition at line 136 of file LTC681x.h.

The documentation for this struct was generated from the following file:

- LTC681x.h