| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
WALLSNS_GOOD
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

WALLSNS_GOOD Bit Field. More...

## Macros
#define | LTC4155_WALLSNS_GOOD_SUBADDR LTC4155_REG4_SUBADDR
| WALLSNS_GOOD More...
#define | LTC4155_WALLSNS_GOOD_SIZE 1
#define | LTC4155_WALLSNS_GOOD_OFFSET 5
#define | LTC4155_WALLSNS_GOOD_MASK 0x20
#define | LTC4155_WALLSNS_GOOD (LTC4155_WALLSNS_GOOD_OFFSET << 12 | (LTC4155_WALLSNS_GOOD_SIZE - 1) << 8 | LTC4155_WALLSNS_GOOD_SUBADDR)

## Detailed Description

WALLSNS_GOOD Bit Field.

WALL input voltage valid.

- Register: REG4
- CommandCode: 0x04
- Size: 1
- Offset: 5
- MSB: 5
- MASK: 0x20
- Access: R
- Default: n/a

## Macro Definition Documentation

## ◆ LTC4155_WALLSNS_GOOD

#define LTC4155_WALLSNS_GOOD (LTC4155_WALLSNS_GOOD_OFFSET << 12 | (LTC4155_WALLSNS_GOOD_SIZE - 1) << 8 | LTC4155_WALLSNS_GOOD_SUBADDR)

Definition at line 637 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLSNS_GOOD_MASK

#define LTC4155_WALLSNS_GOOD_MASK 0x20

Definition at line 636 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLSNS_GOOD_OFFSET

#define LTC4155_WALLSNS_GOOD_OFFSET 5

Definition at line 635 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLSNS_GOOD_SIZE

#define LTC4155_WALLSNS_GOOD_SIZE 1

Definition at line 634 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLSNS_GOOD_SUBADDR

#define LTC4155_WALLSNS_GOOD_SUBADDR LTC4155_REG4_SUBADDR

WALLSNS_GOOD

Definition at line 633 of file LTC4155_reg_defs.h.