| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
ENABLE_INPUT_UVCL_INT
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

ENABLE_INPUT_UVCL_INT Bit Field. More...

## Macros
#define | LTC4155_ENABLE_INPUT_UVCL_INT_SUBADDR LTC4155_REG6_SUBADDR
| ENABLE_INPUT_UVCL_INT More...
#define | LTC4155_ENABLE_INPUT_UVCL_INT_SIZE 1
#define | LTC4155_ENABLE_INPUT_UVCL_INT_OFFSET 2
#define | LTC4155_ENABLE_INPUT_UVCL_INT_MASK 0x04
#define | LTC4155_ENABLE_INPUT_UVCL_INT (LTC4155_ENABLE_INPUT_UVCL_INT_OFFSET << 12 | (LTC4155_ENABLE_INPUT_UVCL_INT_SIZE - 1) << 8 | LTC4155_ENABLE_INPUT_UVCL_INT_SUBADDR)

## Detailed Description

ENABLE_INPUT_UVCL_INT Bit Field.

Enable INPUT_UVCL_ACTIVE interrupts.

- Register: REG6
- CommandCode: 0x06
- Size: 1
- Offset: 2
- MSB: 2
- MASK: 0x04
- Access: R/W
- Default: 0

## Macro Definition Documentation

## ◆ LTC4155_ENABLE_INPUT_UVCL_INT

#define LTC4155_ENABLE_INPUT_UVCL_INT (LTC4155_ENABLE_INPUT_UVCL_INT_OFFSET << 12 | (LTC4155_ENABLE_INPUT_UVCL_INT_SIZE - 1) << 8 | LTC4155_ENABLE_INPUT_UVCL_INT_SUBADDR)

Definition at line 955 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_INPUT_UVCL_INT_MASK

#define LTC4155_ENABLE_INPUT_UVCL_INT_MASK 0x04

Definition at line 954 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_INPUT_UVCL_INT_OFFSET

#define LTC4155_ENABLE_INPUT_UVCL_INT_OFFSET 2

Definition at line 953 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_INPUT_UVCL_INT_SIZE

#define LTC4155_ENABLE_INPUT_UVCL_INT_SIZE 1

Definition at line 952 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_INPUT_UVCL_INT_SUBADDR

#define LTC4155_ENABLE_INPUT_UVCL_INT_SUBADDR LTC4155_REG6_SUBADDR

ENABLE_INPUT_UVCL_INT

Definition at line 951 of file LTC4155_reg_defs.h.