| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Data Fields
t_RECORD_PMBUS_MODIFY_BYTE_NO_PEC Struct Reference

## Detailed Description

Definition at line 666 of file record_type_definitions.h.

## Data Fields
tRecordHeaderLengthAndType | baseRecordHeader
tRecordHeaderAddressAndCommandWithOptionalPEC | detailedRecordHeader
uint8_t | byteMask
uint8_t | desiredDataByte

## Field Documentation

## ◆ baseRecordHeader

tRecordHeaderLengthAndType t_RECORD_PMBUS_MODIFY_BYTE_NO_PEC::baseRecordHeader

Definition at line 668 of file record_type_definitions.h.

## ◆ byteMask

uint8_t t_RECORD_PMBUS_MODIFY_BYTE_NO_PEC::byteMask

Definition at line 670 of file record_type_definitions.h.

## ◆ desiredDataByte

uint8_t t_RECORD_PMBUS_MODIFY_BYTE_NO_PEC::desiredDataByte

Definition at line 671 of file record_type_definitions.h.

## ◆ detailedRecordHeader

tRecordHeaderAddressAndCommandWithOptionalPEC t_RECORD_PMBUS_MODIFY_BYTE_NO_PEC::detailedRecordHeader

Definition at line 669 of file record_type_definitions.h.

The documentation for this struct was generated from the following file:

- record_type_definitions.h