| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - a -

- A_PIN : DC1410AB.ino , DC1410AA.ino
- AC_ADDR_0 : LT3965.h
- ack_error : DC1496BB.ino , DC2156.ino , DC2561.ino , DC1812AA.ino , DC998A.ino , DC2024A.ino , DC1812A-B.ino , DC2217A.ino , DC1697A.ino
- ACTIVE_ANALOG_CUSTOM_ADDRESS_LSB : configuration_constants_LTC2986.h
- ACTIVE_ANALOG_CUSTOM_LENGTH_1_LSB : configuration_constants_LTC2986.h
- ACTIVE_ANALOG_CUSTOM_VALUES_LSB : configuration_constants_LTC2986.h
- ACTIVE_ANALOG_DIFFERENTIAL : configuration_constants_LTC2986.h
- ACTIVE_ANALOG_DIFFERENTIAL_LSB : configuration_constants_LTC2986.h
- ACTIVE_ANALOG_SINGLE_ENDED : configuration_constants_LTC2986.h
- ad7124_handler : EVAL-AD7124-8.ino
- ADAFRUIT_TFT_TOUCHSHIELD_1947 : EasySMU_IOpanel.h
- ADAX : LTC68041.cpp , LTC68042.cpp
- adc_2x : DC939A.ino
- adc_code : DC2071AA.ino
- adc_command : DC2071AA.ino
- ADC_CONVERSION_MODE : DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino
- ADC_DCP : DC2350AA.ino , DC2350AB.ino , DC2515.ino , DC2259.ino
- ADC_HARD_FAILURE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- ADC_MFR_TELEMETRY_STATUS : fast_telemetry.ino
- ADC_OPT : DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino
- ADC_OPT_DISABLED : LTC681x.h
- ADC_OPT_ENABLED : LTC681x.h
- ADC_RANGE_ERROR : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- adc_rejection : DC939A.ino
- adc_voltage : DC2071AA.ino
- ADCOPT : DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino
- ADCV : LTC68041.cpp , LTC68042.cpp
- add64() : LTC6950.h , LTC6945.cpp , LTC6945.h , LTC6946.cpp , LTC6946.h , LTC6947.cpp , LTC6947.h , LTC6948.cpp , LTC6948.h , LTC6950.cpp
- addr2ch : CN0416_capitalizer.ino , CN0416_echo_node.ino
- address : DC2091A.ino
- address1 : LT3965.h
- address2 : LT3965.h
- ADDRESS_DAC_ALL : LTC2752.h , LTC2758.h
- ADDRESS_DACA : LTC2752.h , LTC2758.h
- ADDRESS_DACB : LTC2752.h , LTC2758.h
- address_map : DC579A.ino , DC809A.ino , DC935A.ino , DC934A.ino , DC1466.ino , DC1534A.ino , DC1678A.ino , DC1703A.ino , DC1397A.ino , DC1529A.ino , vmClock.ino
- ADDRx : LTC6954.h , LTC6950.h , LTC6945.h , LTC6946.h , LTC6947.h , LTC6948.h , LTC6951.h , LTC6952.h , LTC6953.h
- adin2_gain : LTM9100.h , DC2423A.ino
- adin_gain : LTM9100.h , DC2423A.ino
- adin_lsb : DC998A.ino
- AFTER_DONE : record_type_definitions.h
- alarms : DC2343A.ino
- alert1_code : DC2156.ino
- alert2_code : DC2156.ino
- alert_code : DC1812A-B.ino , DC1496BB.ino , DC1812AA.ino , DC1697A.ino
- ALERTPIN : LT3965.h
- An0 : DC2218A.ino
- An1 : DC2218A.ino
- An2 : DC2218A.ino
- analog() : DC2218A.ino
- analogAuto() : DC2218A.ino
- analogInPin : LT1054_voltage_mode_buck.ino , LT1054_voltage_mode_buck_DC_ctrl.ino
- analogOutPin : LT1054_voltage_mode_buck.ino , LT1054_voltage_mode_buck_DC_ctrl.ino
- analyze() : Audio_Spectrum_Analyzer.ino
- arduino_spi_modes : platform_drivers.cpp
- AREF : LTC6115.h
- array_size : LTC2442_Datalogger.ino
- ascii_to_hex() : hex_file_parser.cpp
- ask_clear_set_bit() : DC2423A.ino
- assign_channel() : support_functions_LTC2984.h , support_functions_LTC2986.cpp , support_functions_LTC2986.h , support_functions_LTC2983.cpp , support_functions_LTC2983.h , support_functions_LTC2984.cpp
- AUTOMATIC_MODE_DISPLAY_DELAY : DC1496BB.ino , DC1812A-B.ino , DC1812AA.ino
- AUX : LTC6810.h , LTC6812.h , LTC681x.h , LTC6811.h , LTC6813.h
- AUX_CH_ALL : LTC68042.h , LTC681x.h , LTC68041.h
- AUX_CH_GPIO1 : LTC681x.h , LTC68041.h , LTC68042.h
- AUX_CH_GPIO2 : LTC68042.h , LTC68041.h , LTC681x.h
- AUX_CH_GPIO3 : LTC681x.h , LTC68041.h , LTC68042.h
- AUX_CH_GPIO4 : LTC68042.h , LTC681x.h , LTC68041.h
- AUX_CH_GPIO5 : LTC68041.h , LTC681x.h , LTC68042.h
- AUX_CH_TO_CONVERT : DC2350AA.ino , DC2350AB.ino , DC2515.ino , DC2259.ino
- AUX_CH_VREF2 : LTC681x.h , LTC68042.h , LTC68041.h
- aux_codes : DC1894.ino , DC1942.ino
- Av : DC1410AA.ino , DC1410AB.ino
- AVERAGE : SeeedTouchScreen.cpp
- AVERAGETIME : SeeedTouchScreen.cpp
- avr_analog() : SeeedTouchScreen.cpp