| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

### - w -

- wait_for_ack() : retention.ino
- wait_for_not_busy() : retention.ino
- wait_for_nvm() : program.ino
- wait_for_nvm_done() : retention.ino
- wait_for_process_to_finish() : support_functions_LTC2984.h , support_functions_LTC2986.cpp , support_functions_LTC2983.cpp , support_functions_LTC2986.h , support_functions_LTC2983.h , support_functions_LTC2984.cpp
- wait_for_ready() : retention.ino
- wakeup_idle() : LTC681x.cpp , LTC681x.h , LTC68041.cpp , LTC68041.h , LTC68042.cpp , LTC68042.h
- wakeup_sleep() : LTC68041.cpp , LTC68041.h , LTC68042.cpp , LTC68042.h , LTC681x.cpp , LTC681x.h
- wave() : DC2218A.ino
- Wire_Connect() : platform_drivers.cpp , platform_drivers.h
- Wire_Read() : platform_drivers.cpp , platform_drivers.h
- Wire_Write() : platform_drivers.cpp , platform_drivers.h
- write_68() : LTC681x.h , LTC681x.cpp
- write_all() : Synth.ino
- write_bytes() : DC2218A.ino , retention.ino
- write_custom_steinhart_hart() : support_functions_LTC2983.cpp , support_functions_LTC2984.cpp , support_functions_LTC2986.h , support_functions_LTC2984.h , support_functions_LTC2986.cpp , support_functions_LTC2983.h
- write_custom_table() : support_functions_LTC2983.h , support_functions_LTC2986.h , support_functions_LTC2984.cpp , support_functions_LTC2986.cpp , support_functions_LTC2983.cpp , support_functions_LTC2984.h
- write_register() : DC1674A.ino
- writeNvmData() : nvm_data_helpers.cpp , nvm_data_helpers.h