| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
EXT_PWR_GOOD
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

EXT_PWR_GOOD Bit Field. More...

## Macros
#define | LTC4155_EXT_PWR_GOOD_SUBADDR LTC4155_REG4_SUBADDR
| EXT_PWR_GOOD More...
#define | LTC4155_EXT_PWR_GOOD_SIZE 1
#define | LTC4155_EXT_PWR_GOOD_OFFSET 7
#define | LTC4155_EXT_PWR_GOOD_MASK 0x80
#define | LTC4155_EXT_PWR_GOOD (LTC4155_EXT_PWR_GOOD_OFFSET << 12 | (LTC4155_EXT_PWR_GOOD_SIZE - 1) << 8 | LTC4155_EXT_PWR_GOOD_SUBADDR)

## Detailed Description

EXT_PWR_GOOD Bit Field.

External power (Wall or USB) available.

- Register: REG4
- CommandCode: 0x04
- Size: 1
- Offset: 7
- MSB: 7
- MASK: 0x80
- Access: R
- Default: n/a

## Macro Definition Documentation

## ◆ LTC4155_EXT_PWR_GOOD

#define LTC4155_EXT_PWR_GOOD (LTC4155_EXT_PWR_GOOD_OFFSET << 12 | (LTC4155_EXT_PWR_GOOD_SIZE - 1) << 8 | LTC4155_EXT_PWR_GOOD_SUBADDR)

Definition at line 595 of file LTC4155_reg_defs.h.

## ◆ LTC4155_EXT_PWR_GOOD_MASK

#define LTC4155_EXT_PWR_GOOD_MASK 0x80

Definition at line 594 of file LTC4155_reg_defs.h.

## ◆ LTC4155_EXT_PWR_GOOD_OFFSET

#define LTC4155_EXT_PWR_GOOD_OFFSET 7

Definition at line 593 of file LTC4155_reg_defs.h.

## ◆ LTC4155_EXT_PWR_GOOD_SIZE

#define LTC4155_EXT_PWR_GOOD_SIZE 1

Definition at line 592 of file LTC4155_reg_defs.h.

## ◆ LTC4155_EXT_PWR_GOOD_SUBADDR

#define LTC4155_EXT_PWR_GOOD_SUBADDR LTC4155_REG4_SUBADDR

EXT_PWR_GOOD

Definition at line 591 of file LTC4155_reg_defs.h.