| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Data Fields
LT_3887FaultLog::FaultLogPreambleLtc3887 Struct Reference

## Detailed Description

Definition at line 87 of file LT_3887FaultLog.h.

## Data Fields
uint16_t | lt
uint16_t | mfr_special_id
uint8_t | position_fault
struct FaultLogTimeStamp | shared_time
struct FaultLogTelemetrySummaryLtc3887 | peaks

## Field Documentation

## ◆ lt

uint16_t LT_3887FaultLog::FaultLogPreambleLtc3887::lt

Definition at line 90 of file LT_3887FaultLog.h.

## ◆ mfr_special_id

uint16_t LT_3887FaultLog::FaultLogPreambleLtc3887::mfr_special_id

Definition at line 91 of file LT_3887FaultLog.h.

## ◆ peaks

struct FaultLogTelemetrySummaryLtc3887 LT_3887FaultLog::FaultLogPreambleLtc3887::peaks

Definition at line 94 of file LT_3887FaultLog.h.

## ◆ position_fault

uint8_t LT_3887FaultLog::FaultLogPreambleLtc3887::position_fault

Definition at line 92 of file LT_3887FaultLog.h.

## ◆ shared_time

struct FaultLogTimeStamp LT_3887FaultLog::FaultLogPreambleLtc3887::shared_time

Definition at line 93 of file LT_3887FaultLog.h.

The documentation for this struct was generated from the following file:

- LT_3887FaultLog.h