| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Data Fields
t_RECORD_PMBUS_MODIFY_BYTE Struct Reference

## Detailed Description

Definition at line 730 of file record_type_definitions.h.

## Data Fields
tRecordHeaderLengthAndType | baseRecordHeader
tRecordHeaderAddressAndCommandWithOptionalPEC | detailedRecordHeader
uint8_t | byteMask
uint8_t | desiredDataByte

## Field Documentation

## ◆ baseRecordHeader

tRecordHeaderLengthAndType t_RECORD_PMBUS_MODIFY_BYTE::baseRecordHeader

Definition at line 732 of file record_type_definitions.h.

## ◆ byteMask

uint8_t t_RECORD_PMBUS_MODIFY_BYTE::byteMask

Definition at line 734 of file record_type_definitions.h.

## ◆ desiredDataByte

uint8_t t_RECORD_PMBUS_MODIFY_BYTE::desiredDataByte

Definition at line 735 of file record_type_definitions.h.

## ◆ detailedRecordHeader

tRecordHeaderAddressAndCommandWithOptionalPEC t_RECORD_PMBUS_MODIFY_BYTE::detailedRecordHeader

Definition at line 733 of file record_type_definitions.h.

The documentation for this struct was generated from the following file:

- record_type_definitions.h