| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
NTC_WARNING
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

NTC_WARNING Bit Field. More...

## Macros
#define | LTC4155_NTC_WARNING_SUBADDR LTC4155_REG5_SUBADDR
| NTC_WARNING More...
#define | LTC4155_NTC_WARNING_SIZE 1
#define | LTC4155_NTC_WARNING_OFFSET 0
#define | LTC4155_NTC_WARNING_MASK 0x01
#define | LTC4155_NTC_WARNING (LTC4155_NTC_WARNING_OFFSET << 12 | (LTC4155_NTC_WARNING_SIZE - 1) << 8 | LTC4155_NTC_WARNING_SUBADDR)

## Detailed Description

NTC_WARNING Bit Field.

Thermistor temperature out of range for battery charging.

- Register: REG5
- CommandCode: 0x05
- Size: 1
- Offset: 0
- MSB: 0
- MASK: 0x01
- Access: R
- Default: n/a

## Macro Definition Documentation

## ◆ LTC4155_NTC_WARNING

#define LTC4155_NTC_WARNING (LTC4155_NTC_WARNING_OFFSET << 12 | (LTC4155_NTC_WARNING_SIZE - 1) << 8 | LTC4155_NTC_WARNING_SUBADDR)

Definition at line 803 of file LTC4155_reg_defs.h.

## ◆ LTC4155_NTC_WARNING_MASK

#define LTC4155_NTC_WARNING_MASK 0x01

Definition at line 802 of file LTC4155_reg_defs.h.

## ◆ LTC4155_NTC_WARNING_OFFSET

#define LTC4155_NTC_WARNING_OFFSET 0

Definition at line 801 of file LTC4155_reg_defs.h.

## ◆ LTC4155_NTC_WARNING_SIZE

#define LTC4155_NTC_WARNING_SIZE 1

Definition at line 800 of file LTC4155_reg_defs.h.

## ◆ LTC4155_NTC_WARNING_SUBADDR

#define LTC4155_NTC_WARNING_SUBADDR LTC4155_REG5_SUBADDR

NTC_WARNING

Definition at line 799 of file LTC4155_reg_defs.h.