| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - i -

- i2cbus() : LT_SMBus , LT_SMBusBase
- i2cbus_ : LT_SMBusBase
- Iadc_code_ : EasySMU
- ic_reg : cell_asic
- id : gpio_desc , i2c_desc , i2c_init_param , spi_desc , spi_init_param
- Idac_pulldown_code_ : EasySMU
- Idac_pullup_code_ : EasySMU
- iin_data : LT_2975FaultLog::FaultLogReadLoopLtc2975
- iin_peaks : LT_2975FaultLog::FaultLogPeaksLtc2975
- immediateOff() : LT_PMBus , LT_PMBusRail
- immediateOffGlobal() : LT_PMBus
- Init() : EasySMU_IOpanel
- initButton() : Adafruit_GFX_Button
- invertDisplay() : Adafruit_GFX , Adafruit_ILI9341
- iout0_peaks : LT_2974FaultLog::FaultLogPeaksLtc2974 , LT_2975FaultLog::FaultLogPeaksLtc2975
- iout1_peaks : LT_2974FaultLog::FaultLogPeaksLtc2974 , LT_2975FaultLog::FaultLogPeaksLtc2975
- iout2_peaks : LT_2974FaultLog::FaultLogPeaksLtc2974 , LT_2975FaultLog::FaultLogPeaksLtc2975
- iout3_peaks : LT_2974FaultLog::FaultLogPeaksLtc2974 , LT_2975FaultLog::FaultLogPeaksLtc2975
- iout_data0 : LT_2974FaultLog::FaultLogReadLoopLtc2974 , LT_2975FaultLog::FaultLogReadLoopLtc2975
- iout_data1 : LT_2974FaultLog::FaultLogReadLoopLtc2974 , LT_2975FaultLog::FaultLogReadLoopLtc2975
- iout_data2 : LT_2974FaultLog::FaultLogReadLoopLtc2974 , LT_2975FaultLog::FaultLogReadLoopLtc2975
- iout_data3 : LT_2974FaultLog::FaultLogReadLoopLtc2974 , LT_2975FaultLog::FaultLogReadLoopLtc2975
- is_a_temperature_measurement : channel_table
- isController() : LT_PMBusRail
- isLtc2974() : LT_PMBus
- isLtc2977() : LT_PMBus
- isLtc2978() : LT_PMBus
- isLtc297x() : LT_PMBus
- isMultiphase() : LT_PMBusRail
- isospi_reverse : cell_asic
- IsPresent() : EasySMU
- isPressed() : Adafruit_GFX_Button
- isTouching() : TouchScreen
- isValidData() : LT_2974FaultLog::FaultLogLtc2974 , LT_2975FaultLog::FaultLogLtc2975 , LT_2977FaultLog::FaultLogLtc2977 , LT_2978FaultLog::FaultLogLtc2978