| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Public Member Functions | Data Fields
LT_2975FaultLog::FaultLogLtc2975 Struct Reference

## Detailed Description

Definition at line 220 of file LT_2975FaultLog.h.

## Public Member Functions
bool | isValidData (void *pos, uint8_t size=2)

## Data Fields
struct FaultLogPreambleLtc2975 | preamble
uint8_t | telemetryData [176]
struct FaultLogReadLoopLtc2975 * | loops
uint8_t | firstValidByte
uint8_t | lastValidByte

## Member Function Documentation

## ◆ isValidData()

bool LT_2975FaultLog::FaultLogLtc2975::isValidData | ( | void * | pos,
|  | uint8_t | size = `2`
| ) |  |

Definition at line 77 of file LT_2975FaultLog.cpp.

## Field Documentation

## ◆ firstValidByte

uint8_t LT_2975FaultLog::FaultLogLtc2975::firstValidByte

Definition at line 226 of file LT_2975FaultLog.h.

## ◆ lastValidByte

uint8_t LT_2975FaultLog::FaultLogLtc2975::lastValidByte

Definition at line 227 of file LT_2975FaultLog.h.

## ◆ loops

struct FaultLogReadLoopLtc2975* LT_2975FaultLog::FaultLogLtc2975::loops

Definition at line 225 of file LT_2975FaultLog.h.

## ◆ preamble

struct FaultLogPreambleLtc2975 LT_2975FaultLog::FaultLogLtc2975::preamble

Definition at line 223 of file LT_2975FaultLog.h.

## ◆ telemetryData

uint8_t LT_2975FaultLog::FaultLogLtc2975::telemetryData[176]

Definition at line 224 of file LT_2975FaultLog.h.

The documentation for this struct was generated from the following files:

- LT_2975FaultLog.h
- LT_2975FaultLog.cpp