| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
LOWBAT
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

LOWBAT Bit Field. More...

## Macros
#define | LTC4155_LOWBAT_SUBADDR LTC4155_REG3_SUBADDR
| LOWBAT More...
#define | LTC4155_LOWBAT_SIZE 1
#define | LTC4155_LOWBAT_OFFSET 0
#define | LTC4155_LOWBAT_MASK 0x01
#define | LTC4155_LOWBAT (LTC4155_LOWBAT_OFFSET << 12 | (LTC4155_LOWBAT_SIZE - 1) << 8 | LTC4155_LOWBAT_SUBADDR)

## Detailed Description

LOWBAT Bit Field.

Battery below ~2.8V or charger disabled.

- Register: REG3
- CommandCode: 0x03
- Size: 1
- Offset: 0
- MSB: 0
- MASK: 0x01
- Access: R
- Default: n/a

## Macro Definition Documentation

## ◆ LTC4155_LOWBAT

#define LTC4155_LOWBAT (LTC4155_LOWBAT_OFFSET << 12 | (LTC4155_LOWBAT_SIZE - 1) << 8 | LTC4155_LOWBAT_SUBADDR)

Definition at line 549 of file LTC4155_reg_defs.h.

## ◆ LTC4155_LOWBAT_MASK

#define LTC4155_LOWBAT_MASK 0x01

Definition at line 548 of file LTC4155_reg_defs.h.

## ◆ LTC4155_LOWBAT_OFFSET

#define LTC4155_LOWBAT_OFFSET 0

Definition at line 547 of file LTC4155_reg_defs.h.

## ◆ LTC4155_LOWBAT_SIZE

#define LTC4155_LOWBAT_SIZE 1

Definition at line 546 of file LTC4155_reg_defs.h.

## ◆ LTC4155_LOWBAT_SUBADDR

#define LTC4155_LOWBAT_SUBADDR LTC4155_REG3_SUBADDR

LOWBAT

Definition at line 545 of file LTC4155_reg_defs.h.