| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
ID_PIN_DETECT
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

ID_PIN_DETECT Bit Field. More...

## Macros
#define | LTC4155_ID_PIN_DETECT_SUBADDR LTC4155_REG3_SUBADDR
| ID_PIN_DETECT More...
#define | LTC4155_ID_PIN_DETECT_SIZE 1
#define | LTC4155_ID_PIN_DETECT_OFFSET 4
#define | LTC4155_ID_PIN_DETECT_MASK 0x10
#define | LTC4155_ID_PIN_DETECT (LTC4155_ID_PIN_DETECT_OFFSET << 12 | (LTC4155_ID_PIN_DETECT_SIZE - 1) << 8 | LTC4155_ID_PIN_DETECT_SUBADDR)

## Detailed Description

ID_PIN_DETECT Bit Field.

On-the-Go boost ID pin detection status.

- Register: REG3
- CommandCode: 0x03
- Size: 1
- Offset: 4
- MSB: 4
- MASK: 0x10
- Access: R
- Default: n/a

## Macro Definition Documentation

## ◆ LTC4155_ID_PIN_DETECT

#define LTC4155_ID_PIN_DETECT (LTC4155_ID_PIN_DETECT_OFFSET << 12 | (LTC4155_ID_PIN_DETECT_SIZE - 1) << 8 | LTC4155_ID_PIN_DETECT_SUBADDR)

Definition at line 482 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ID_PIN_DETECT_MASK

#define LTC4155_ID_PIN_DETECT_MASK 0x10

Definition at line 481 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ID_PIN_DETECT_OFFSET

#define LTC4155_ID_PIN_DETECT_OFFSET 4

Definition at line 480 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ID_PIN_DETECT_SIZE

#define LTC4155_ID_PIN_DETECT_SIZE 1

Definition at line 479 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ID_PIN_DETECT_SUBADDR

#define LTC4155_ID_PIN_DETECT_SUBADDR LTC4155_REG3_SUBADDR

ID_PIN_DETECT

Definition at line 478 of file LTC4155_reg_defs.h.