| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
REQUEST_OTG
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

REQUEST_OTG Bit Field. More...

## Macros
#define | LTC4155_REQUEST_OTG_SUBADDR LTC4155_REG6_SUBADDR
| REQUEST_OTG More...
#define | LTC4155_REQUEST_OTG_SIZE 1
#define | LTC4155_REQUEST_OTG_OFFSET 1
#define | LTC4155_REQUEST_OTG_MASK 0x02
#define | LTC4155_REQUEST_OTG (LTC4155_REQUEST_OTG_OFFSET << 12 | (LTC4155_REQUEST_OTG_SIZE - 1) << 8 | LTC4155_REQUEST_OTG_SUBADDR)

## Detailed Description

REQUEST_OTG Bit Field.

USB On-The-Go step-up voltage converter manual activation setting.

- Register: REG6
- CommandCode: 0x06
- Size: 1
- Offset: 1
- MSB: 1
- MASK: 0x02
- Access: R/W
- Default: 0

## Macro Definition Documentation

## ◆ LTC4155_REQUEST_OTG

#define LTC4155_REQUEST_OTG (LTC4155_REQUEST_OTG_OFFSET << 12 | (LTC4155_REQUEST_OTG_SIZE - 1) << 8 | LTC4155_REQUEST_OTG_SUBADDR)

Definition at line 976 of file LTC4155_reg_defs.h.

## ◆ LTC4155_REQUEST_OTG_MASK

#define LTC4155_REQUEST_OTG_MASK 0x02

Definition at line 975 of file LTC4155_reg_defs.h.

## ◆ LTC4155_REQUEST_OTG_OFFSET

#define LTC4155_REQUEST_OTG_OFFSET 1

Definition at line 974 of file LTC4155_reg_defs.h.

## ◆ LTC4155_REQUEST_OTG_SIZE

#define LTC4155_REQUEST_OTG_SIZE 1

Definition at line 973 of file LTC4155_reg_defs.h.

## ◆ LTC4155_REQUEST_OTG_SUBADDR

#define LTC4155_REQUEST_OTG_SUBADDR LTC4155_REG6_SUBADDR

REQUEST_OTG

Definition at line 972 of file LTC4155_reg_defs.h.