| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
INPUT_UVCL_ACTIVE
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

INPUT_UVCL_ACTIVE Bit Field. More...

## Macros
#define | LTC4155_INPUT_UVCL_ACTIVE_SUBADDR LTC4155_REG4_SUBADDR
| INPUT_UVCL_ACTIVE More...
#define | LTC4155_INPUT_UVCL_ACTIVE_SIZE 1
#define | LTC4155_INPUT_UVCL_ACTIVE_OFFSET 3
#define | LTC4155_INPUT_UVCL_ACTIVE_MASK 0x08
#define | LTC4155_INPUT_UVCL_ACTIVE (LTC4155_INPUT_UVCL_ACTIVE_OFFSET << 12 | (LTC4155_INPUT_UVCL_ACTIVE_SIZE - 1) << 8 | LTC4155_INPUT_UVCL_ACTIVE_SUBADDR)

## Detailed Description

INPUT_UVCL_ACTIVE Bit Field.

Input undervoltage limit control circuit engaged (brownout).

- Register: REG4
- CommandCode: 0x04
- Size: 1
- Offset: 3
- MSB: 3
- MASK: 0x08
- Access: R
- Default: n/a

## Macro Definition Documentation

## ◆ LTC4155_INPUT_UVCL_ACTIVE

#define LTC4155_INPUT_UVCL_ACTIVE (LTC4155_INPUT_UVCL_ACTIVE_OFFSET << 12 | (LTC4155_INPUT_UVCL_ACTIVE_SIZE - 1) << 8 | LTC4155_INPUT_UVCL_ACTIVE_SUBADDR)

Definition at line 679 of file LTC4155_reg_defs.h.

## ◆ LTC4155_INPUT_UVCL_ACTIVE_MASK

#define LTC4155_INPUT_UVCL_ACTIVE_MASK 0x08

Definition at line 678 of file LTC4155_reg_defs.h.

## ◆ LTC4155_INPUT_UVCL_ACTIVE_OFFSET

#define LTC4155_INPUT_UVCL_ACTIVE_OFFSET 3

Definition at line 677 of file LTC4155_reg_defs.h.

## ◆ LTC4155_INPUT_UVCL_ACTIVE_SIZE

#define LTC4155_INPUT_UVCL_ACTIVE_SIZE 1

Definition at line 676 of file LTC4155_reg_defs.h.

## ◆ LTC4155_INPUT_UVCL_ACTIVE_SUBADDR

#define LTC4155_INPUT_UVCL_ACTIVE_SUBADDR LTC4155_REG4_SUBADDR

INPUT_UVCL_ACTIVE

Definition at line 675 of file LTC4155_reg_defs.h.