| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
ENABLE_AT_ILIM_INT
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

ENABLE_AT_ILIM_INT Bit Field. More...

## Macros
#define | LTC4155_ENABLE_AT_ILIM_INT_SUBADDR LTC4155_REG6_SUBADDR
| ENABLE_AT_ILIM_INT More...
#define | LTC4155_ENABLE_AT_ILIM_INT_SIZE 1
#define | LTC4155_ENABLE_AT_ILIM_INT_OFFSET 3
#define | LTC4155_ENABLE_AT_ILIM_INT_MASK 0x08
#define | LTC4155_ENABLE_AT_ILIM_INT (LTC4155_ENABLE_AT_ILIM_INT_OFFSET << 12 | (LTC4155_ENABLE_AT_ILIM_INT_SIZE - 1) << 8 | LTC4155_ENABLE_AT_ILIM_INT_SUBADDR)

## Detailed Description

ENABLE_AT_ILIM_INT Bit Field.

Enable AT_INPUT_ILIM interrupts.

- Register: REG6
- CommandCode: 0x06
- Size: 1
- Offset: 3
- MSB: 3
- MASK: 0x08
- Access: R/W
- Default: 0

## Macro Definition Documentation

## ◆ LTC4155_ENABLE_AT_ILIM_INT

#define LTC4155_ENABLE_AT_ILIM_INT (LTC4155_ENABLE_AT_ILIM_INT_OFFSET << 12 | (LTC4155_ENABLE_AT_ILIM_INT_SIZE - 1) << 8 | LTC4155_ENABLE_AT_ILIM_INT_SUBADDR)

Definition at line 934 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_AT_ILIM_INT_MASK

#define LTC4155_ENABLE_AT_ILIM_INT_MASK 0x08

Definition at line 933 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_AT_ILIM_INT_OFFSET

#define LTC4155_ENABLE_AT_ILIM_INT_OFFSET 3

Definition at line 932 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_AT_ILIM_INT_SIZE

#define LTC4155_ENABLE_AT_ILIM_INT_SIZE 1

Definition at line 931 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_AT_ILIM_INT_SUBADDR

#define LTC4155_ENABLE_AT_ILIM_INT_SUBADDR LTC4155_REG6_SUBADDR

ENABLE_AT_ILIM_INT

Definition at line 930 of file LTC4155_reg_defs.h.