| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
ENABLE_FAULT_INT
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

ENABLE_FAULT_INT Bit Field. More...

## Macros
#define | LTC4155_ENABLE_FAULT_INT_SUBADDR LTC4155_REG6_SUBADDR
| ENABLE_FAULT_INT More...
#define | LTC4155_ENABLE_FAULT_INT_SIZE 1
#define | LTC4155_ENABLE_FAULT_INT_OFFSET 6
#define | LTC4155_ENABLE_FAULT_INT_MASK 0x40
#define | LTC4155_ENABLE_FAULT_INT (LTC4155_ENABLE_FAULT_INT_OFFSET << 12 | (LTC4155_ENABLE_FAULT_INT_SIZE - 1) << 8 | LTC4155_ENABLE_FAULT_INT_SUBADDR)

## Detailed Description

ENABLE_FAULT_INT Bit Field.

Enable OVP_ACTIVE, OTG_FAULT, BAD_CELL, and NTCSTAT = Hot_Fault interrupts.

- Register: REG6
- CommandCode: 0x06
- Size: 1
- Offset: 6
- MSB: 6
- MASK: 0x40
- Access: R/W
- Default: 0

## Macro Definition Documentation

## ◆ LTC4155_ENABLE_FAULT_INT

#define LTC4155_ENABLE_FAULT_INT (LTC4155_ENABLE_FAULT_INT_OFFSET << 12 | (LTC4155_ENABLE_FAULT_INT_SIZE - 1) << 8 | LTC4155_ENABLE_FAULT_INT_SUBADDR)

Definition at line 871 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_FAULT_INT_MASK

#define LTC4155_ENABLE_FAULT_INT_MASK 0x40

Definition at line 870 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_FAULT_INT_OFFSET

#define LTC4155_ENABLE_FAULT_INT_OFFSET 6

Definition at line 869 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_FAULT_INT_SIZE

#define LTC4155_ENABLE_FAULT_INT_SIZE 1

Definition at line 868 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ENABLE_FAULT_INT_SUBADDR

#define LTC4155_ENABLE_FAULT_INT_SUBADDR LTC4155_REG6_SUBADDR

ENABLE_FAULT_INT

Definition at line 867 of file LTC4155_reg_defs.h.